{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":11,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM40M2V1B","2AMXM50M2V1B","2AMXM50M4V1B","2AMXM50M3V1B"]
["Puhallin","Ilmamäärä","Jäähdytys","Erittäin pieni","m³/min","","","30","34"]
["","","Lämmitys","Erittäin pieni","m³/min","","","32","34"]
["Äänen tehotaso","Lämmitys","","","dBA","","62","","","62"]
["","Jäähdytys","","","dBA","","60","","","60"]
["Puhallin","Ilmamäärä","Jäähdytys","Erittäin pieni","cfm","","","1059","1200"]
["","","Lämmitys","Erittäin pieni","cfm","","","1130","1200"]
["Mitat","Yksikkö","","Korkeus","mm","550","550","550","550","550","550"]
["","","","Leveys","mm","765","765","765","765","765","765"]
["","","","Syvyys","mm","285","285","285","285","285","285"]
["Paino","Yksikkö","","","kg","36","36","36","41","41","41"]
["Puhallinmoottori","Nopeus","Jäähdytys","Erittäin pieni","r/min","500","500","760","890","500","500"]
["","","Lämmitys","Erittäin pieni","r/min","320","320","820","890","500","500"]
["Kompressori","Type","","","","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori","","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","","46.0","-10","-10","46.0"]
["","","","Maks.","°CDB","","-10","46","46","-10"]
["","Lämmitys","Ympäristö","Min.","°CWB","","-15","-15","-15","-15.0"]
["","","","Maks.","°CWB","","18.0","18","18","18.0"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","46","46","","","48","48"]
["","","","Nimell.","dBA","","","48","46"]
["","Lämmitys","","Suuri","dBA","48","48","","","50","50"]
["","","","Nimell.","dBA","","","50","48"]
["Kylmäaine","Tyyppi","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Täytösmäärä","","","kg","0.88","0.88","0.88","1.15","1.15","1.15"]
["","Täytösmäärä","","","tCO2Eq","0.59","0.6","0.6","0.8","0.78","0.78"]
["","GWP","","","","675.0","675","675","675","675","675"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","20","20 (1)","20","20","20 (1)","20"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 20 m putkistoille)","0,02 (yli 20 m putkistoille)","002 (yli 20 m putkistoille)","0,02 (yli 20 m putkistoille)","0,02 (yli 20 m putkistoille)","0,02 (yli 20 m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","15.0","15","15","15","15","15.0"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5","7.5","7.5","7.5"]
["","Putkiston kokonaispituus","Järjestelmä","Todellinen","m","30","30","30","30","30","30"]
["Vakiovarusteet","Installation manual","","","","1","1","Installation manual","1","1","1"]
["","Drain plug","","","","1","1","Drain plug","1","1","1"]
["","Screw bag","","","","1","1","Screw bag","1","1","1"]
["Virransyöttö","Vaihe","","","","1~","1~","1~","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50","50","50","50"]
["","Jännite","","","V","220-230-240","220-230-240","220-240","220-240","220-230-240","220-230-240"]
["Huomautukset","","","","","(1) - Yhdelle huoneelle","","(1) - Sisältää fluorattuja kasvihuonekaasuja","","","(1) - Yhdelle huoneelle"]
["","","","","","","(1) - Yhdelle huoneelle","","","(1) - Yhdelle huoneelle"]
["","","","","","","(2) - Katso toimintalämpötila-alue eri piirustuksesta","","","(2) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","","","(3) - Katso sähköiset tiedot eri piirustuksista","","","(3) - Katso sähköiset tiedot eri piirustuksista"]
["","","","","","","(4) - Sisältää fluorattuja kasvihuonekaasuja","","","(4) - Sisältää fluorattuja kasvihuonekaasuja"]
["Kompressori","Tyyppi","","","","","","Hermeettisesti suljettu swing-kompressori"]
["Vakiovarusteet","Reducer assembly","","","","","","","1","1","1"]