{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-N"]
[]
[]
[]
[]
["","","","","","2MXM40N2V1B","2MXM50N2V1B","2MXM68N2V1B"]
["Mitat","Yksikkö","","Korkeus","mm","550","550","734"]
["","","","Leveys","mm","765","765","958"]
["","","","Syvyys","mm","285","285","340"]
["Paino","Yksikkö","","","kg","36","41","60"]
["Puhallinmoottori","Nopeus","Jäähdytys","Erittäin pieni","r/min","500","500","420"]
["","","Lämmitys","Erittäin pieni","r/min","320","500","420"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","","","-10"]
["","","","Maks.","°CDB","","","46"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","46","48"]
["","","","Nimell.","dBA","","","48"]
["","Lämmitys","","Suuri","dBA","48","50"]
["","","","Nimell.","dBA","","","48.0"]
["Kylmäaine","Tyyppi","","","","R-32","R-32","R-32"]
["","Täytösmäärä","","","kg","0.88","1.15","2"]
["","Täytösmäärä","","","tCO2Eq","0.60","0.78","1.35"]
["","GWP","","","","675","675","675.0"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","20","20","25"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 20 m putkistoille)","0,02 (yli 20 m putkistoille)","0,02 (yli 30m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","15.0","15.0","15.0"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5"]
["","Putkiston kokonaispituus","Järjestelmä","Todellinen","m","30","30","50"]
["Vakiovarusteet","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Virransyöttö","Vaihe","","","","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50"]
["","Jännite","","","V","220-230-240","220-230-240","220-240"]
["Huomautukset","","","","","(1) - Yhdelle huoneelle","(1) - Yhdelle huoneelle","(1) - Yhdelle huoneelle"]
["Vakiovarusteet","Reducer assembly","","","","","1","1"]
["","Drain cap","","","","","","3"]