{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B2","2MXS40H3V1B","2MXS40H2V1B","2MXS50H3V1B2","2MXS50H3V1B","2MXS50H2V1B"]
["Äänenpaineen taso","Lämmitys","","Nimell.","dBA","48","48","","50","50"]
["","Jäähdytys","","Nimell.","dBA","47","47","","48","48"]
["Vakiovarusteet","Asennusohje","","","","1","1","","1","1"]
["","Ruuvipussi","","","","1","1","","1","1"]
["","Tyhjennystulppa","","","","1","1","","1","1"]
["Kylmäaine","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Täytösmäärä","","","kg","1.20","1.20","","1.60","1.60"]
["","Tyyppi","","","","R-410A","R-410A","","R-410A","R-410A"]
["Putkiliitännät","Korkeusero","IU - IU","Maks.","m","7.5","7.5","","7.5","7.5"]
["","","IU - OU","Maks.","m","15","15","","15","15"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 20 m putkistoille)","0,02 (yli 20 m putkistoille)","","0,02 (yli 20 m putkistoille)","0,02 (yli 20 m putkistoille)"]
["","Putkiston kokonaispituus","Järjestelmä","Todellinen","m","30","30","","30","30"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu keinukompressori","Hermeettisesti suljettu keinukompressori","","Hermeettisesti suljettu keinukompressori","Hermeettisesti suljettu keinukompressori"]
["Mitat","Yksikkö","","Leveys","mm","765","765","","765","765"]
["","","","Syvyys","mm","285","285","","285","285"]
["","","","Korkeus","mm","550","550","","550","550"]
["Paino","Yksikkö","","","kg","38","38","","42","42"]
["Power supply","Vaihe","","","","1~","1~","","1~","1~"]
["","Taajuus","","","Hz","50","50","","50","50"]
["","Jännite","","","V","220-240","220-240","","220-240","220-240"]
["Huomautukset","","","","","(1) - Sisältää fluorattuja kasvihuonekaasuja","(1) - Sisältää fluorattuja kasvihuonekaasuja","","(1) - Sisältää fluorattuja kasvihuonekaasuja","(1) - Sisältää fluorattuja kasvihuonekaasuja"]
["Mitat","Yksikkö","","Korkeus","mm","","","550","","","550"]
["","","","Leveys","mm","","","765","","","765"]
["","","","Syvyys","mm","","","285","","","285"]
["Paino","Yksikkö","","","kg","","","38","","","42"]
["Kompressori","Tyyppi","","","","","","Hermeettisesti suljettu swing-kompressori","","","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","","","10","","","10"]
["","","","Maks.","°CDB","","","46","","","46"]
["","Lämmitys","Ympäristö","Min.","°CWB","","","-15","","","-15"]
["","","","Maks.","°CWB","","","15.5","","","15.5"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","","","47","","","48"]
["","Lämmitys","","Nimell.","dBA","","","48","","","50"]
["Kylmäaine","Tyyppi","","","","","","R-410A","","","R-410A"]
["","Täytösmäärä","","","kg","","","1.20","","","1.60"]
["","Täytösmäärä","","","tCO2Eq","","","2.5","","","3.3"]
["","GWP","","","","","","2087.5","","","2087.5"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","","","20","","","20"]
["","Lisäkylmäainemäärä","","","kg/m","","","0,02 (yli 20 m putkistoille)","","","0,02 (yli 20 m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","","","15","","","15"]
["","","IU - IU","Maks.","m","","","7.5","","","7.5"]
["","Putkiston kokonaispituus","Järjestelmä","Todellinen","m","","","30","","","30"]
["Vakiovarusteet","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Virransyöttö","Vaihe","","","","","","1~","","","1~"]
["Syöttöjännite","Taajuus","","","Hz","","","50","","","50"]
["","Jännite","","","V","","","220-240","","","220-240"]
["Vakiovarusteet","Supistuskokoonpano","","","","","","","1","1"]
["","Reducer assembly","","","","","","","","","1"]