{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Äänenpaineen taso","Lämmitys","","Nimell.","dBA","47"]
["","Jäähdytys","","Nimell.","dBA","46"]
["Vakiovarusteet","Asennusohje","","","","1"]
["","Ruuvipussi","","","","1"]
["","Tyhjennystulppa","","","","1"]
["","Tyhjennyskorkki (1)","","","","6"]
["","Tyhjennyskorkki (2)","","","","3"]
["","Irrotettava F-kaasun merkintä","","","","1"]
["","Lisäkylmäaineen merkintä","","","","1"]
["Kylmäaine","Charge","","","TCO2Eq","1.2"]
["","GWP","","","","675"]
["","Charge","","","kg","1.8"]
["","Tyyppi","","","","R-32"]
["Puhallinmoottori","Nopeus","Jäähdytys","Erittäin pieni","r/min","420"]
["","","Lämmitys","Erittäin pieni","r/min","420"]
["Putkiliitännät","Korkeusero","IU - IU","Maks.","m","7.5"]
["","","IU - OU","Maks.","m","15"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 30m putkistoille)"]
["","Putkiston kokonaispituus","Järjestelmä","Todellinen","m","50"]
["Compressor","Type","","","","Hermeettisesti suljettu keinukompressori"]
["Mitat","Yksikkö","","Leveys","mm","868"]
["","","","Syvyys","mm","320"]
["","","","Korkeus","mm","734"]
["Paino","Yksikkö","","","kg","57"]
["Power supply","Vaihe","","","","1~"]
["","Taajuus","","","Hz","50"]
["","Jännite","","","V","220-240"]
["Huomautukset","","","","","(1) - Sisältää fluorattuja kasvihuonekaasuja"]
["","","","","","(2) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","","(3) - Katso sähköiset tiedot eri piirustuksista"]
["Puhallin","Ilmamäärä","Jäähdytys","Erittäin pieni","m³/min","","24"]
["","","Lämmitys","Erittäin pieni","m³/min","","24"]
["","","","Erittäin pieni","cfm","","847"]
["","","Lämmitys","Erittäin pieni","cfm","","847"]
["Mitat","Yksikkö","","Korkeus","mm","","734"]
["","","","Leveys","mm","","868"]
["","","","Syvyys","mm","","320"]
["Paino","Yksikkö","","","kg","","57"]
["Puhallinmoottori","Nopeus","Jäähdytys","Erittäin pieni","r/min","","420"]
["","","Lämmitys","Erittäin pieni","r/min","","420"]
["Compressor","Type","","","","","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","","-10"]
["","","","Maks.","°CDB","","46"]
["","Lämmitys","Ympäristö","Min.","°CWB","","-15"]
["","","","Maks.","°CWB","","18"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","","46"]
["","Lämmitys","","Nimell.","dBA","","47"]
["Kylmäaine","Tyyppi","","","","","R-32"]
["","Täytösmäärä","","","kg","","1.80"]
["","Täytösmäärä","","","tCO2Eq","","1.2"]
["","GWP","","","","","675"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","","25"]
["","Lisäkylmäainemäärä","","","kg/m","","0,02 (yli 30m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","","15"]
["","","IU - IU","Maks.","m","","7.5"]
["","Putkiston kokonaispituus","Järjestelmä","Todellinen","m","","50"]
["Vakiovarusteet","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["Virransyöttö","Vaihe","","","","","1~"]
["Syöttöjännite","Taajuus","","","Hz","","50"]
["","Jännite","","","V","","220-240"]