{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-M"]
[]
[]
[]
[]
["","","","","","3MXM40M2V1B","3MXM52M2V1B","3MXM68M2V1B"]
["Puhallin","Ilmamäärä","Jäähdytys","Erittäin pieni","m³/min","24","24","24.1"]
["","","Lämmitys","Erittäin pieni","m³/min","24","24","24.1"]
["","","","Erittäin pieni","cfm","847","847","851"]
["","","Lämmitys","Erittäin pieni","cfm","847","847","851"]
["Mitat","Yksikkö","","Korkeus","mm","734","734","734"]
["","","","Leveys","mm","868","868","868"]
["","","","Syvyys","mm","320","320","320"]
["Paino","Yksikkö","","","kg","57","57","62"]
["Puhallinmoottori","Nopeus","Jäähdytys","Erittäin pieni","r/min","420","420"]
["","","Lämmitys","Erittäin pieni","r/min","420","420"]
["Kompressori","Type","","","","Hermeettisesti suljettu swing-kompressori","","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46"]
["","Lämmitys","Ympäristö","Min.","°CWB","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","46","46","48"]
["","Lämmitys","","Nimell.","dBA","47","47","48"]
["Kylmäaine","Tyyppi","","","","R-32","R-32","R-32"]
["","Täytösmäärä","","","kg","1.80","1.80","2.0"]
["","Täytösmäärä","","","tCO2Eq","1.2","1.2","1.4"]
["","GWP","","","","675","675","675"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","25","25","25"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 30m putkistoille)","0,02 (yli 30m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","15","15","15"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5"]
["","Putkiston kokonaispituus","Järjestelmä","Todellinen","m","50","50"]
["Vakiovarusteet","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Virransyöttö","Vaihe","","","","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50"]
["","Jännite","","","V","220-240","220-240","220-240"]
["Kompressori","Tyyppi","","","","","Hermeettisesti suljettu swing-kompressori"]
["Vakiovarusteet","Drain cap","","","","","","9"]
["","Reducer assembly","","","","","","1"]