{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N7"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B7","3MXM52N2V1B7","3MXM68N2V1B7"]
["Puhallin","Ilmamäärä","Jäähdytys","Erittäin pieni","m³/min","","","24.1"]
["","","Lämmitys","Erittäin pieni","m³/min","","","24.1"]
["","","","Erittäin pieni","cfm","","","851"]
["","","Lämmitys","Erittäin pieni","cfm","","","851"]
["Mitat","Yksikkö","","Korkeus","mm","734","734","734"]
["","","","Leveys","mm","974","974","958"]
["","","","Syvyys","mm","401","401","340"]
["Paino","Yksikkö","","","kg","57","57","62"]
["Puhallinmoottori","Nopeus","Jäähdytys","Erittäin pieni","r/min","420","420"]
["","","Lämmitys","Erittäin pieni","r/min","420","420"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46"]
["","Lämmitys","Ympäristö","Min.","°CWB","","","-15"]
["","","","Maks.","°CWB","","","24"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","46","46","48"]
["","Lämmitys","","Nimell.","dBA","47","47","48"]
["Kylmäaine","Tyyppi","","","","R-32","R-32","R-32"]
["","Täytösmäärä","","","kg","1.8","1.8","2"]
["","Täytösmäärä","","","tCO2Eq","1.22","1.22"]
["","GWP","","","","675","675","675"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","25","25 (1)","25"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 30m putkistoille)","0,02 (yli 30m putkistoille)","002 (yli 30m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","15.0","15.0","15"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5"]
["","Putkiston kokonaispituus","Järjestelmä","Todellinen","m","50","50 (2)","50"]
["Vakiovarusteet","Installation manual","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["","Reducer assembly","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Virransyöttö","Vaihe","","","","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50"]
["","Jännite","","","V","220-240","220-240","220-440"]
["Huomautukset","","","","","(1) - Yhdelle huoneelle","(1) - Yhdelle huoneelle"]
["","","","","","(2) - Yhdistelmäksi malleihin CVXM-A, FVXM-A - putkiston enimmäispituus on 30m.","(2) - Yhdistelmäksi malleihin CVXM-A, FVXM-A - putkiston enimmäispituus on 30m."]
["Kompressori","Tyyppi","","","","","","Hermeettisesti suljettu swing-kompressori"]
["Energiatehokkuusalue","","","","","","","A+++ ~ D"]