{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MWXM-A9"]
[]
[]
[]
[]
["","","","","","5MWXM68A2V1B9","5MWXM90A2V1B9"]
["Mitat","Yksikkö","","Korkeus","mm","734","734"]
["","","","Leveys","mm","1,040","1,040"]
["","","","Syvyys","mm","408","408"]
["Paino","Yksikkö","","","kg","69","73"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","48","52"]
["","Lämmitys","","Nimell.","dBA","49","53"]
["Kylmäaine","Tyyppi","","","","R-32","R-32"]
["","Täytösmäärä","","","kg","2","2.4"]
["","Täytösmäärä","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","25 (2)","25 (3)"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 30m putkistoille)","0,02 (yli 30m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","15 (3)","15"]
["","","IU - IU","Maks.","m","7.5 (3)","7.5 (3)"]
["","Putkiston kokonaispituus","Järjestelmä","Todellinen","m","60","75"]
["Vakiovarusteet","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","2","2"]
["Virransyöttö","Vaihe","","","","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50"]
["","Jännite","","","V","220-440","220-240"]
["Huomautukset","","","","","(1) - Katso toimintalämpötila-alue eri piirustuksesta","(1) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","","(2) - Yhdelle huoneelle","(2) - Yhdelle huoneelle"]
["","","","","","(3) - Yhteen huoneeseen (yhdistelmälle mallien FBA71/100/125 sekä EKHWET ja CKHWS kanssa katso asennusohje)","(3) - Yhteen huoneeseen (yhdistelmälle mallien FBA71/100/125 sekä EKHWET ja CKHWS kanssa katso asennusohje)"]
["","","","","","(4) - Sisältää fluorattuja kasvihuonekaasuja","(4) - Sisältää fluorattuja kasvihuonekaasuja"]