{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-A"]
[]
[]
[]
[]
["","","","","","5MXM90A2V1B"]
["Mitat","Yksikkö","","Korkeus","mm","734"]
["","","","Leveys","mm","974"]
["","","","Syvyys","mm","408"]
["Paino","Yksikkö","","","kg","68"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-10"]
["","","","Maks.","°CDB","46"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","52"]
["","Lämmitys","","Nimell.","dBA","52"]
["Kylmäaine","Tyyppi","","","","R-32"]
["","Täytösmäärä","","","kg","2.4"]
["","Täytösmäärä","","","tCO2Eq","1.62"]
["","GWP","","","","675"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","25 (1)"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 30m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","15"]
["","","IU - IU","Maks.","m","7.5"]
["","Putkiston kokonaispituus","Järjestelmä","Todellinen","m","75"]
["Vakiovarusteet","Installation manual","","","","1"]
["","Drain cap","","","","3"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Virransyöttö","Vaihe","","","","1~"]
["Syöttöjännite","Taajuus","","","Hz","50"]
["","Jännite","","","V","220-240"]
["Huomautukset","","","","","(1) - Yhdelle huoneelle"]