{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C / AZQS-BY1"]
[]
[]
[]
[]
["","","","","ABQ100CV1 / AZQS100B7Y1B","ABQ125CV1 / AZQS125B7Y1B"]
["Jäähdytysteho","Nimell.","","kW","9.5","12.1 (1)"]
["Tilan jäähdytys","SEER","","","4.65","4.68"]
["","Vuotuinen energiankulutus","","kWh/a","716","1,550"]
["","Teho","Pdesign","kW","9.50","12.1"]
["","Energiatehokkuusluokka","","","B"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Teho","Pdesign","kW","6.78","8.13"]
["","SCOP/A","","","3.80","3.41"]
["","Energiatehokkuusluokka","","","A"]
["","Vuotuinen energiankulutus","","kWh/a","2,498","3,340"]
["Nimellinen tehokkuus","Vuotuinen energiankulutus","","kWh","1,813"]
["","EER","","","2.62","2.27 (3)"]
["","COP","","","3.42"]
["","Energiamerkintädirektiivi","Jäähdytys","","D"]
["","","Lämmitys","","B"]
["Lämmitysteho","Nimell.","","kW","10.8","13.5 (2)"]
["Huomautukset","","","","(1) - EER/COP Eurovent 2012 -standardin mukaan, käytettäväksi ainoastaan EU:n ulkopuolella","(1) - Jäähdytys: sisälämpötila 27°CDB, 19°CWB, ulkolämpötila 35°CDB; putkiston ekvivalenttipituus: 7,5 m; korkeusero: 0m"]
["","","","","(2) - Vuotuinen energiankulutus ilmoitettu energiamerkintää koskevan direktiivin 2002/31/EY mukaisesti","(2) - Lämmitys: sisälämpötila 20°CDB; ulkolämpötila 7°CDB, 6°CWB, kylmäaineputkiston ekvivalenttipituus: 7,5 m; korkeusero: 0m"]
["","","","","(3) - SEER ja SCOP ovat EN 14825:n mukaiset","(3) - EER/COP Eurovent 2012 -standardin mukaan, käytettäväksi ainoastaan EU:n ulkopuolella"]
["","","","","(4) - Nimellinen tehokkuus: jäähdytys 35°/27° nimelliskuormalla, lämmitys 7°/20° nimelliskuormalla"]