{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Vakiovarusteet","Asennusohje","","","","Asennusohje"]
["","Käyttöopas","","","","Käyttöopas"]
["","Ruuvi + aluslevy","","","","Ruuvi + aluslevy"]
["","Langaton kaukosäädin","","","","Langaton kaukosäädin"]
["","Säleikön lukitus","","","","Säleikön lukitus"]
["","Paristo","","","","Paristo"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","9.52"]
["","Kaasu","","Ulkohalkaisija","mm","15.88"]
["","Tyhjennys","","","","19.05"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.128"]
["","Lämmitys","","Nimell.","kW","0.128"]
["Sound power level","Jäähdytys","","","dBA","64"]
["","Lämmitys","","","dBA","64"]
["Mitat","Yksikkö","","Leveys","mm","600"]
["","","","Syvyys","mm","1,007"]
["","","","Korkeus","mm","285"]
["Kotelo","Materiaali","","","","Galvanoitu teräs"]
["Paino","Unit","","","kg","35"]
["Puhallin","Ulkoinen staattinen paine","","Suuri","Pa","90"]
["","","","Nim.","Pa","77"]
["","","","Pieni","Pa","64"]
["Power supply","Vaihe","","","","1~"]
["","Taajuus","","","Hz","50"]
["","Nimi","","","","V1"]
["","Jännite","","","V","220-240"]
["Ottoteho","Lämmitys","","Nimell.","kW","","0.109"]
["","Jäähdytys","","Nimell.","kW","","0.109"]
["Puhallin","Ulkoinen staattinen paine","","Suuri","Pa","","70","150","150"]
["","","","Pieni","Pa","","45","111","92"]
["Kotelo","Materiaali","","","","","Galvanoitu teräs"]
["Mitat","Yksikkö","","Korkeus","mm","","378","378","378"]
["","","","Leveys","mm","","541","1300","1500"]
["","","","Syvyys","mm","","1045","541","541"]
["Paino","Yksikkö","","","kg","","44","50","56"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","","22.7","40.5","48.7"]
["","","","Nimell.","m³/min","","20.5","37","44"]
["","","","Pieni","m³/min","","18.3","34.8","37.9"]
["","","Lämmitys","Suuri","m³/min","","22.7","40.5","48.7"]
["","","","Nimell.","m³/min","","20.5","37.4","43.9"]
["","","","Pieni","m³/min","","18.3","34.8","37.9"]
["","Ulkoinen staattinen paine","","Nim.","Pa","","57","128","122"]
["Äänen tehotaso","Jäähdytys","","","dBA","","60","72","73"]
["","Lämmitys","","","dBA","","60","72","73"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","","41","53","55"]
["","","","Nimell.","dBA","","38"]
["","","","Pieni","dBA","","36","50","50"]
["","Lämmitys","","Suuri","dBA","","41","53","55"]
["","","","Nimell.","dBA","","38"]
["","","","Pieni","dBA","","36","50","50"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","","9.52","9.52","9.52"]
["","Kaasu","","Ulkohalkaisija","mm","","15.88","15.9","15.9"]
["","Kondenssi","","","","","19.05"]
["Vakiovarusteet","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Virransyöttö","Vaihe","","","","","1~"]
["Syöttöjännite","Taajuus","","","Hz","","50"]
["","Jännite","","","V","","220-240"]
["Jäähdytysteho","Kokonaisteho","","Nimell.","kW","","","12.10","13.00"]
["Lämmitysteho","Yhteisteho","","Nim.","kW","","","13.5","15.5"]
["Kotelo","Väri","","","","","","Galvanoitu teräslevy / maalaamaton","Galvanoitu teräslevy / maalaamaton"]
["Puhallin","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","","","37","44"]
["","","Lämmitys","Keski","m³/min","","","37.4","43.9"]
["Äänenpaineen taso","Jäähdytys","","Keski","dBA","","","52","53"]
["","Lämmitys","","Keski","dBA","","","52","53"]
["Ohjausjärjestelmät","Infrapuna kaukosäädin","","","","","","ARCWLA","ARCWLA"]