{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1 (Archived)","ACQ100DV1 (Archived)","ACQ125DV1 (Archived)","ACQ140DV1 (Archived)"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","","44","","47"]
["","","","Nimell.","dBA","","41","","44"]
["","","","Hiljainen toiminta","dBA","","36","","41"]
["","","","Pieni","dBA","","38","","43"]
["","Jäähdytys","","Hiljainen toiminta","dBA","","36","","41"]
["","","","Pieni","dBA","","38","","43"]
["","","","Suuri","dBA","","44","","47"]
["","","","Nimell.","dBA","","41","","44"]
["Vakiovarusteet","Asennusohje","","","","","Asennusohje","","Asennusohje"]
["","Käyttöopas","","","","","Käyttöopas","","Käyttöopas"]
["","Ruuvit","","","","","Ruuvit","","Ruuvit"]
["","Aluslevy","","","","","Aluslevy","","Aluslevy"]
["","Langaton kaukosäädin","","","","","Langaton kaukosäädin","","Langaton kaukosäädin"]
["","Säleikön lukitus","","","","","Säleikön lukitus","","Säleikön lukitus"]
["","Paristo","","","","","Paristo","","Paristo"]
["Control systems","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Piping connections","Neste","","Ulkohalkaisija","mm","","9.52","","9.52"]
["","Kaasu","","Ulkohalkaisija","mm","","15.88","","15.88"]
["","Tyhjennys","","","","","19.05","","19.05"]
["Ottoteho","Jäähdytys","","Nimell.","kW","","0.094","","0.137"]
["","Lämmitys","","Nimell.","kW","","0.094","","0.137"]
["Äänen tehotaso","Jäähdytys","","","dBA","","56","","60"]
["","Lämmitys","","","dBA","","56","","60"]
["Mitat","Yksikkö","","Leveys","mm","","820","","820"]
["","","","Syvyys","mm","","820","","820"]
["","","","Korkeus","mm","","300","","300"]
["Casing","Material","","","","","Galvanoitu teräs","","Galvanoitu teräs"]
["Paino","Yksikkö","","","kg","","39","","39"]
["Puhallin","Ilmamäärä","Lämmitys","Suuri","m³/min","","29.2","","34.0"]
["","","","Pieni","m³/min","","21.0","","26.3"]
["","","","Nimell.","m³/min","","24.4","","29.2"]
["","","Cooling","Pieni","m³/min","","21.0","","26.3"]
["","","","Nimell.","m³/min","","24.4","","29.2"]
["","","","Suuri","m³/min","","29.2","","34.0"]
["","","","Hiljainen toiminta","m³/min","","17.6","","22.1"]
["","","Cooling","Hiljainen toiminta","m³/min","","17.6","","22.1"]
["Säleikkö","Paino","","","kg","","4","","4"]
["","Mitat","","Korkeus","mm","","82","","82"]
["","","","Syvyys","mm","","990","","990"]
["","","","Leveys","mm","","990","","990"]
["","Väri","","","","","Valkoinen","","Valkoinen"]
["Power supply","Phase","","","","","1~","","1~"]
["","Name","","","","","V1","","V1"]
["","Taajuus","","","Hz","","50","","50"]
["","Jännite","","","V","","220-240","","220-240"]
["Puhallin","Ilmamäärä","Lämmitys","Hiljainen toiminta","m³/min","15","","22.1"]
["Ottoteho","Lämmitys","","Nimell.","kW","0.067","","0.137"]
["","Jäähdytys","","Nimell.","kW","0.067","","0.137"]
["Puhallin","Ilmamäärä","Jäähdytys","Hiljainen toiminta","m³/min","15","","22.1"]
["Kotelo","Materiaali","","","","Galvanoitu teräs","","Galvanoitu teräs"]
["Mitat","Yksikkö","","Korkeus","mm","265","","300"]
["","","","Leveys","mm","820","","820"]
["","","","Syvyys","mm","820","","820"]
["Paino","Yksikkö","","","kg","31","","39"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","24.4","","34"]
["","","","Nimell.","m³/min","20.5","","29.2"]
["","","","Pieni","m³/min","17.6","","26.3"]
["","","Lämmitys","Suuri","m³/min","24.4","","34"]
["","","","Nimell.","m³/min","20.5","","29.2"]
["","","","Pieni","m³/min","17.6","","26.3"]
["Äänen tehotaso","Jäähdytys","","","dBA","54","","60"]
["","Lämmitys","","","dBA","54","","60"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","41","","47"]
["","","","Nimell.","dBA","38","","44"]
["","","","Pieni","dBA","35","","43"]
["","","","Hiljainen toiminta","dBA","32","","41"]
["","Lämmitys","","Suuri","dBA","41","","47"]
["","","","Nimell.","dBA","38","","44"]
["","","","Pieni","dBA","35","","43"]
["","","","Hiljainen toiminta","dBA","32","","41"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","9.52","","9.52"]
["","Kaasu","","Ulkohalkaisija","mm","15.88","","15.88"]
["","Kondenssi","","","","19.05","","19.05"]
["Säleikkö","Mitat","","Korkeus","mm","82","","82"]
["","","","Leveys","mm","990","","990"]
["","","","Syvyys","mm","990","","990"]
["","Paino","","","kg","4","","4"]
["Ohjausjärjestelmät","Infrapuna kaukosäädin","","","","ARCWLA","","ARCWLA"]
["","Langallinen kaukosäädin","","","","ARCWB","","ARCWB"]
["Vakiovarusteet","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Virransyöttö","Vaihe","","","","1~","","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","","50"]
["","Jännite","","","V","220-240","","220-240"]