{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ADEA100A2VEB / AZQS100B8V1B","ADEA125A2VEB / AZQS125B8V1B"]
["Jäähdytysteho","Nimell.","","kW","9.50","12.10"]
["Tilan jäähdytys","SEER","","","5.10","4.83"]
["","Vuotuinen energiankulutus","","kWh/a","652","1,504"]
["","Teho","Pdesign","kW","9.50","12.10"]
["","Energiatehokkuusluokka","","","A"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Teho","Pdesign","kW","7.60","7.93"]
["","SCOP/A","","","3.81","3.50"]
["","Energiatehokkuusluokka","","","A"]
["","Vuotuinen energiankulutus","","kWh/a","2,793","3,167"]
["Nimellinen tehokkuus","EER","","","","2.27"]
["Lämmitysteho","Nimell.","","kW","10.80","13.50"]
["Huomautukset","","","","(1) - Katso toimintalämpötila-alue eri piirustuksesta","(1) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","(2) - Katso sähköiset tiedot eri piirustuksista","(2) - Katso sähköiset tiedot eri piirustuksista"]
["","","","","(3) - Jäähdytys: sisälämpötila 27°CDB, 19°CWB, ulkolämpötila 35°CDB; putkiston ekvivalenttipituus: 7,5 m; korkeusero: 0m","(3) - Jäähdytys: sisälämpötila 27°CDB, 19°CWB, ulkolämpötila 35°CDB; putkiston ekvivalenttipituus: 7,5 m; korkeusero: 0m"]
["","","","","(4) - Lämmitys: sisälämpötila 20°CDB; ulkolämpötila 7°CDB, 6°CWB, kylmäaineputkiston ekvivalenttipituus: 7,5 m; korkeusero: 0m","(4) - Lämmitys: sisälämpötila 20°CDB; ulkolämpötila 7°CDB, 6°CWB, kylmäaineputkiston ekvivalenttipituus: 7,5 m; korkeusero: 0m"]