{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":11,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A"]
[]
[]
[]
[]
["","","","","","ADEA35A2VEB","ADEA50A2VEB","ADEA60A2VEB","ADEA71A2VEB","ADEA100A2VEB","ADEA125A2VEB"]
["Puhallin","Ulkoinen staattinen paine","","Suuri","Pa","150","150","150","150","150","150"]
["Jäähdytysteho","Kokonaisteho","","Nimell.","kW","","","","","","14.00"]
["Lämmitysteho","Yhteisteho","","Nim.","kW","","","","","","13.50"]
["Kotelo","Väri","","","","Maalaamaton (galvanoitu)","Maalaamaton (galvanoitu)","Maalaamaton (galvanoitu)","Maalaamaton (galvanoitu)","Maalaamaton (galvanoitu)","Maalaamaton (galvanoitu)"]
["","Materiaali","","","","Galvanoitu teräslevy","Galvanoitu teräslevy","Galvanoitu teräslevy","Galvanoitu teräslevy","Galvanoitu teräslevy","Galvanoitu teräslevy"]
["Mitat","Yksikkö","","Korkeus","mm","245","245","245","245","245","245"]
["","","","Leveys","mm","700","700","1000","1000","1400","1400"]
["","","","Syvyys","mm","800","800","800","800","800","800"]
["Paino","Yksikkö","","","kg","28","28","35","35","46","46"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","15","15","18","18","29","34"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","12.5","12.5","15","15","26","29"]
["","","","Pieni","m³/min","10.5","10.5","12.5","12.5","23","23.5"]
["","","Lämmitys","Suuri","m³/min","15","15","18","18","29","34"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","12.5","12.5","15","15","26","29"]
["","","Lämmitys","Pieni","m³/min","10.5","10.5","12.5","12.5","23","23.5"]
["","Ulkoinen staattinen paine","","Nim.","Pa","30","30","30","30","40","50"]
["Äänen tehotaso","Jäähdytys","","","dBA","60","60","56","56","58","62"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","35","35","30","30","34","37"]
["","","","Keski","dBA","32","32","28","28","32","35"]
["","","","Pieni","dBA","29","29","25","25","30","32"]
["","Lämmitys","","Suuri","dBA","37","37","31","31","36","38"]
["","","","Keski","dBA","34","34","28","28","33","35"]
["","","","Pieni","dBA","29","29","25","25","30","32"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35","6.35","6.35","9.52","9.52","9.52"]
["","Kaasu","","Ulkohalkaisija","mm","9.52","12.7","12.7","15.9","15.9","15.9"]
["","Kondenssi","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Nostokorkeus","mm","","","","625","625","625","625","625","625"]
["Ohjausjärjestelmät","Infrapuna kaukosäädin","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["","Langallinen kaukosäädin","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Vakiovarusteet","Installation manual","","","","1","1","1","","1","1"]
["","Washer for hanger bracket","","","","8","8","8","","8","8"]
["","Operation manual","","","","1","1","1","","1","1"]
["","Clamps","","","","4","4","4","","4","4"]
["","Drain hose","","","","1","1","1","","1","1"]
["","Insulation for fitting","","","","2","2","2","","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","","1","1"]
["","Screws","","","","40","40","40","","40","40"]
["","Sealing pads","","","","5","5","5","","5","5"]
["Virransyöttö","Vaihe","","","","1~","1~","1~","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50","50","50","50"]
["","Jännite","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Huomautukset","","","","","","","","(1) - Äänen tehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon.","(1) - Äänen tehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon.","(1) - Äänen tehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon."]
["","","","","","","","","(2) - Katso sähköiset tiedot eri piirustuksista","(2) - Katso sähköiset tiedot eri piirustuksista","(2) - Katso sähköiset tiedot eri piirustuksista"]
["Vakiovarusteet","Asennusohje","","","","","","","1"]
["","Koukkukiinnikkeen aluslevy","","","","","","","8"]
["","Käyttöopas","","","","","","","1"]
["","Siteet","","","","","","","4"]
["","Tyhjennysletku","","","","","","","1"]
["","Asennuseriste","","","","","","","2"]
["","Tyhjennysletkun metallikiristin","","","","","","","1"]
["","Ruuvit","","","","","","","40"]
["","Tiivistysläpät","","","","","","","5"]