{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":9,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Ottoteho","Lämmitys","","Nimell.","kW","0.106","0.149"]
["","Jäähdytys","","Nimell.","kW","0.106","0.149"]
["Puhallin","Ulkoinen staattinen paine","","Suuri","Pa","0","0","0","0"]
["","","","Pieni","Pa","0","0","0","0"]
["Jäähdytysteho","Kokonaisteho","","Nimell.","kW","","","12.10","13.00"]
["Lämmitysteho","Yhteisteho","","Nim.","kW","","","13.5","15.5"]
["Kotelo","Väri","","","","Valkoinen","Valkoinen","Valkoinen","Valkoinen"]
["","Materiaali","","","","Galvanoitu teräs","Galvanoitu teräs"]
["Mitat","Yksikkö","","Korkeus","mm","260","260","260","285"]
["","","","Leveys","mm","1320","1538","1790","1900"]
["","","","Syvyys","mm","634","634","634","680"]
["Paino","Yksikkö","","","kg","38","45","65","70"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nimell.","m³/min","21.3","27.8","31","39"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","","","31","39"]
["","","","Pieni","m³/min","18.9","24.8","27.2","28.3"]
["","","Lämmitys","Suuri","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nimell.","m³/min","21.3","27.8","30.6","39.1"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","","","30.6","39.1"]
["","","Lämmitys","Pieni","m³/min","18.9","24.8","27.2","28.3"]
["","Ulkoinen staattinen paine","","Nim.","Pa","0","0","0","0"]
["Äänen tehotaso","Jäähdytys","","","dBA","59","64","65","71"]
["","Lämmitys","","","dBA","62","64","65","71"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","49","52","52","56"]
["","","","Nimell.","dBA","48","47"]
["","","","Keski","dBA","","","50","53"]
["","","","Pieni","dBA","46","46","49","46"]
["","Lämmitys","","Suuri","dBA","49","52","52","56"]
["","","","Keski","dBA","","","50","53"]
["","","","Nimell.","dBA","48","47"]
["","","","Pieni","dBA","46","46","49","46"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","9.52","9.52","9.52","9.52"]
["","Kaasu","","Ulkohalkaisija","mm","15.88","15.88","15.9","15.9"]
["","Kondenssi","","","","19.05","19.05"]
["Ohjausjärjestelmät","Infrapuna kaukosäädin","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","Langallinen kaukosäädin","","","","ARCWB","ARCWB"]
["Vakiovarusteet","Installation manual","","","","Installation manual","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Battery","","","","Battery","Battery"]
["","Tyhjennysputki","","","","Drain pipe","Drain pipe"]
["","Screw for wireless remote","","","","Screw for wireless remote","Screw for wireless remote"]
["","Ferrite Core","","","","Ferrite Core","Ferrite Core"]
["","Installation manual (Ferrite Core)","","","","Installation manual (Ferrite Core)","Installation manual (Ferrite Core)"]
["","Outdoor wiring diagram","","","","Outdoor wiring diagram","Outdoor wiring diagram"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Drain hose","","","","Drain hose","Drain hose"]
["Virransyöttö","Vaihe","","","","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50"]
["","Jännite","","","V","220-240","220-240"]