{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":10,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-A"]
[]
[]
[]
[]
["","","","","","ARXM25A5V1B","ARXM35A5V1B","ARXM50A5V1B","ARXM60A5V1B","ARXM71A5V1B"]
["Mitat","Yksikkö","","Korkeus","mm","610","610","734","734","734"]
["","","","Leveys","mm","923","923","954","954","954"]
["","","","Syvyys","mm","367","367","401","401","401"]
["Paino","Yksikkö","","","kg","36","36","49","49","49"]
["Puhallinmoottori","Nopeus","Jäähdytys","Erittäin pieni","r/min","600","600","500"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-10","-10","-10","-10","-10"]
["","","","Maks.","°CDB","50","50","50 (1), 46 (1)","46","46"]
["","Lämmitys","Ympäristö","Min.","°CWB","-21","-21","-21 (1), -15 (1)","-15","-15"]
["","","","Maks.","°CWB","18","18","18","18","18"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","46","47","48","48","52"]
["","Lämmitys","","Nimell.","dBA","47","49","49","49","52"]
["Kylmäaine","Tyyppi","","","","R-32","R-32","R-32","R-32","R-32"]
["","Täytösmäärä","","","kg","0.95","0.95","1.1","1.15","1.15"]
["","Täytösmäärä","","","tCO2Eq","0.65","0.65","0.75","0.78","0.78"]
["","GWP","","","","675","675","675","675","675"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","20","20","30","30","30"]
["","Lisäkylmäainemäärä","","","kg/m","002 (yli 10m putkistoille)","002 (yli 10m putkistoille)","002 (yli 10m putkistoille)","002 (yli 10m putkistoille)","0035 (yli 10m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","15","15","20","20","20"]
["Vakiovarusteet","Installation manual","","","","1","1","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","1","3","3"]
["Energiatehokkuusalue","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Virransyöttö","Vaihe","","","","1~","1~","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50","50","50"]
["","Jännite","","","V","220-240","220-240","220-240","220-240","220-240"]
["Huomautukset","","","","","(1) - Katso toimintalämpötila-alue eri piirustuksesta","(1) - Katso toimintalämpötila-alue eri piirustuksesta","(1) - Katso toimintalämpötila-alue eri piirustuksesta","(1) - Katso toimintalämpötila-alue eri piirustuksesta","(1) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","","(2) - Katso sähköiset tiedot eri piirustuksista","(2) - Katso sähköiset tiedot eri piirustuksista","(2) - Katso sähköiset tiedot eri piirustuksista","(2) - Katso sähköiset tiedot eri piirustuksista","(2) - Katso sähköiset tiedot eri piirustuksista"]
["","","","","","(3) - Sisältää fluorattuja kasvihuonekaasuja","(3) - Sisältää fluorattuja kasvihuonekaasuja","(3) - Sisältää fluorattuja kasvihuonekaasuja","(3) - Sisältää fluorattuja kasvihuonekaasuja","(3) - Sisältää fluorattuja kasvihuonekaasuja"]
["Vakiovarusteet","ARXM50A5V1B","","","","","","1"]
["","Drain plug","","","","","","","1","1"]