{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-M"]
[]
[]
[]
[]
["","","","","","ARXM50MV1B","ARXM25M2V1B (Archived)","ARXM35M2V1B (Archived)"]
["Mitat","Yksikkö","","Korkeus","mm","735","550","550"]
["","","","Leveys","mm","825","765","765"]
["","","","Syvyys","mm","300","285","285"]
["Paino","Yksikkö","","","kg","44","32","32"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46"]
["","Lämmitys","Ympäristö","Min.","°CWB","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","48","46","49"]
["","","","Pieni","dBA","44"]
["","Lämmitys","","Suuri","dBA","49","47","49"]
["","","","Pieni","dBA","45"]
["Kylmäaine","Tyyppi","","","","R-32","R-32","R-32"]
["","Täytösmäärä","","","kg","1.4","0.76","0.76"]
["","Täytösmäärä","","","tCO2Eq","0.9","0.5","0.5"]
["","GWP","","","","675","675","675"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","30","15","15"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 10m putkistoille)","0,02 (yli 10m putkistoille)","0,02 (yli 10m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","20","12","12"]
["Vakiovarusteet","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1"]
["Virransyöttö","Vaihe","","","","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50"]
["","Jännite","","","V","220-240","220-240","220-240"]