{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Äänenpaineen taso","Lämmitys","","Nimell.","dBA","","49.0"]
["","Jäähdytys","","Nimell.","dBA","","49.0"]
["Vakiovarusteet","Tyhjennystulppa","","","","","1"]
["","Asennusohje","","","","","1"]
["","Kylmäaineen määrän tarra","","","","","1"]
["","Monikieliset fluorattujen kasvihuonekaasujen merkinnät","","","","","1"]
["","Yleiset varotoimet","","","","","1"]
["Kylmäaine","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Täytösmäärä","","","kg","","0.76"]
["","Type","","","","","R-32"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Maks.","°CDB","","50 (4), 46 (5)"]
["","","","Min.","°CDB","","-10"]
["Piping connections","Korkeusero","IU - OU","Maks.","m","","15"]
["","Lisäkylmäainemäärä","","","kg/m","","0,02 (yli 10m putkistoille)"]
["Kompressori","Tyyppi","","","","","Hermeettisesti suljettu keinukompressori"]
["Mitat","Yksikkö","","Leveys","mm","","840"]
["","","","Syvyys","mm","","350"]
["","","","Korkeus","mm","","552"]
["Paino","Yksikkö","","","kg","","32"]
["Power supply","Phase","","","","","1~"]
["","Taajuus","","","Hz","","50"]
["","Jännite","","","V","","220-240"]
["Huomautukset","","","","","(1) - Mahdollinen vain yhdistämällä ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Sisältää fluorattuja kasvihuonekaasuja"]
["","","","","","(2) - Mahdollinen vain yhdistämällä ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","","","(3) - Katso sähköiset tiedot eri piirustuksista"]
["","","","","","","(4) - Mahdollinen vain yhdistämällä ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Mahdollinen vain yhdistämällä ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Mitat","Yksikkö","","Korkeus","mm","552"]
["","","","Leveys","mm","840"]
["","","","Syvyys","mm","350"]
["Paino","Yksikkö","","","kg","32"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-10"]
["","","","Maks.","°CDB","50 (4), 46 (5)"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","46.0"]
["","Lämmitys","","Nimell.","dBA","47.0"]
["Kylmäaine","Täytösmäärä","","","kg","0.76"]
["","Täytösmäärä","","","tCO2Eq","0.52"]
["","GWP","","","","675"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","20"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 10m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","15"]
["Vakiovarusteet","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Syöttöjännite","Taajuus","","","Hz","50"]