{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","","48"]
["","","","Pieni","dBA","","45"]
["Vakiovarusteet","1","","","","","550"]
["Kylmäaine","Charge","","","kg","","2.5"]
["","Tyyppi","","","","","1.2"]
["Puhallin","Ilmamäärä","Jäähdytys","Erittäin pieni","m³/min","","30.1"]
["","","","Erittäin pieni","cfm","","1,063"]
["Puhallinmoottori","Nopeus","Jäähdytys","Erittäin pieni","r/min","","740"]
["","","Lämmitys","Erittäin pieni","r/min","","-15"]
["Toimintalämpötila-alue","Heating","Ympäristö","Min.","°CWB","","20"]
["","","","Maks.","°CWB","","10"]
["Äänenpaineen taso","Jäähdytys","","Pieni","dBA","","44"]
["","","","Suuri","dBA","","48"]
["Compressor","Tyyppi","","","","","Hermeettisesti suljettu keinukompressori"]
["Mitat","Yksikkö","","Leveys","mm","","285"]
["","","","Syvyys","mm","","612"]
["","","","Korkeus","mm","","765"]
["Paino","Yksikkö","","","kg","","34"]
["Puhallin","Ilmamäärä","Lämmitys","Erittäin pieni","cfm","","904"]
["","","","Erittäin pieni","m³/min","","25.6"]
["Power supply","Vaihe","","","","","1~"]
["","Taajuus","","","Hz","","50"]
["","Jännite","","","V","","220-240"]
["Huomautukset","","","","","(1) - 220 V","(1) - Sisältää fluorattuja kasvihuonekaasuja"]
["","","","","","(2) - 230 V","(2) - 220 V"]
["","","","","","(3) - 240 V","(3) - 230 V"]
["","","","","","","(4) - 240 V"]
["Puhallin","Ilmamäärä","Jäähdytys","Erittäin pieni","m³/min","30.1"]
["","","Lämmitys","Erittäin pieni","m³/min","25.6"]
["","","","Erittäin pieni","cfm","1063"]
["","","Lämmitys","Erittäin pieni","cfm","904"]
["Mitat","Yksikkö","","Korkeus","mm","550"]
["","","","Leveys","mm","765"]
["","","","Syvyys","mm","285"]
["Paino","Yksikkö","","","kg","34"]
["Puhallinmoottori","Nopeus","Jäähdytys","Erittäin pieni","r/min","780"]
["","","Lämmitys","Erittäin pieni","r/min","740"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","10"]
["","","","Maks.","°CDB","46"]
["","Lämmitys","Ympäristö","Min.","°CWB","-15"]
["","","","Maks.","°CWB","18"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","46"]
["","Lämmitys","","Suuri","dBA","47"]
["","","","Pieni","dBA","44"]
["Kylmäaine","Tyyppi","","","","R-410A"]
["","Täytösmäärä","","","kg","1.0"]
["","Täytösmäärä","","","tCO2Eq","2.1"]
["","GWP","","","","2087.5"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","20"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 10m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","15"]
["Vakiovarusteet","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Virransyöttö","Vaihe","","","","1~"]
["Syöttöjännite","Taajuus","","","Hz","50"]
["","Jännite","","","V","220-240"]