{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":12,"n_cols":14,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATB"]
[]
[]
[]
[]
["","","","","SB.ATB05LBM","SB.ATB05RBM","SB.ATB06LBM","SB.ATB06RBM","SB.ATB07LBM","SB.ATB07RBM","ATB03LBMNADBT00","ATB03RBMNADBT00","ATB04LBMNADBT00","ATB04RBMNADBT00"]
["Nimellinen ilmanvirtaus","Paluuilman virtaus","","m³/s","0.639","0.639","0.750","0.750","1.083","1.083","0.222","0.222","0.458","0.458"]
["","Syöttöilmanvirtaus","","m³/s","0.639","0.639","0.75","0.75","1.083","1.083","0.222","0.222","0.458","0.458"]
["Mitat","Yksikkö","Korkeus","mm","1750","1750","1700","1700","1900","1900","1450","1450","1450","1450"]
["","","Leveys","mm","790","790","790","790","890","890","550","550","790","790"]
["","","Pituus vaimentimella","mm","2170","2170","2620","2620","2950","2950","1580","1580","1650","1650"]
["Syöttösuodatin","Ensiösuodatin","Luokka","","F7","F7","F7","F7","F7","F7","F7","F7","F7","F7"]