{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":11,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K2V1B","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B","ATX35K2V1B (Archived)"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","","","","","","43"]
["","","","Keski","dBA","","","","","","35"]
["","","","Hiljainen toiminta","dBA","","","","","","26"]
["","","","Pieni","dBA","","","","","","29"]
["","Jäähdytys","","Keski","dBA","","","","","","34"]
["","","","Hiljainen toiminta","dBA","","","","","","20"]
["","","","Pieni","dBA","","","","","","27"]
["","","","Suuri","dBA","","","","","","43"]
["Vakiovarusteet","Asennusohje","","","","","","","","","1"]
["","Käyttöopas","","","","","","","","","1"]
["","Infrapunakauko-ohjain","","","","","","","","","1"]
["","AA-kuivaparistot","","","","","","","","","2"]
["","Kaukosäätimen pidike","","","","","","","","","1"]
["","Kiinnityslevy","","","","","","","","","1"]
["","Fotokatalyyttinen titaani-apatiitti-ilmanpuhdistussuodatin","","","","","","","","","2"]
["","Sisäyksikön kiinnitysruuvit","","","","","","","","","2"]
["Ohjausjärjestelmät","Wired remote control","","","","","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","","","","","ARC480A11"]
["Putkistoliitännät","Neste","","Ulkohalkaisija","mm","","","","","","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","","","","","","9.50"]
["","Tyhjennys","","","","","","","","","18"]
["Ottoteho","Jäähdytys","","Nimell.","kW","","","","","","0.024"]
["","Lämmitys","","Nimell.","kW","","","","","","0.029"]
["Sound power level","Jäähdytys","","","dBA","","","","","","58"]
["","Lämmitys","","","dBA","","","","","","58"]
["Mitat","Yksikkö","","Leveys","mm","","","","","","770"]
["","","","Syvyys","mm","","","","","","225"]
["","","","Korkeus","mm","","","","","","286"]
["Kotelo","Väri","","","","","","","","","Valkoinen"]
["Paino","Yksikkö","","","kg","","","","","","9.0"]
["Power supply","Vaihe","","","","","","","","","1~"]
["","Taajuus","","","Hz","","","","","","50"]
["","Nimi","","","","","","","","","V1"]
["","Jännite","","","V","","","","","","220-240"]
["Huomautukset","","","","","","","","","","(1) - SL: Ilmanvirtausasetuksen hiljainen asetus puhaltimelle"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.018","0.018","0.02","0.02","0.024"]
["","Lämmitys","","Nimell.","kW","0.022","0.022","0.023","0.023","0.029"]
["Kotelo","Väri","","","","Valkoinen","Valkoinen","Valkoinen","Valkoinen","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","286","286","286","286","286"]
["","","","Leveys","mm","770","770","770","770","770"]
["","","","Syvyys","mm","225","225","225","225","225"]
["Paino","Yksikkö","","","kg","8.5","8.5","8.5","8.5","9"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","9.9","9.9","10.4","10.4","11.8"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","7.8","7.8","8","8","8.2"]
["","","","Pieni","m³/min","5.8","5.8","6.1","6.1","6.3"]
["","","","Hiljainen toiminta","m³/min","4.8","4.8","4.8","4.8","4.9"]
["","","Lämmitys","Suuri","m³/min","10.9","10.9","11.1","11.1","12.8"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","8.5","8.5","8.5","8.5","8.5"]
["","","Lämmitys","Pieni","m³/min","6.4","6.4","6.7","6.7","6.9"]
["","","","Hiljainen toiminta","m³/min","5.2","5.2","5.2","5.2","5.2"]
["Äänen tehotaso","Jäähdytys","","","dBA","55","55","55","55","58"]
["","Lämmitys","","","dBA","55","55","55","55","58"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","39","39","40","40","43"]
["","","","Keski","dBA","33","33","33","33","34"]
["","","","Pieni","dBA","25","25","26","26","27"]
["","","","Hiljainen toiminta","dBA","20","20","20","20","20"]
["","Lämmitys","","Suuri","dBA","39","39","40","40","43"]
["","","","Keski","dBA","34","34","34","34","35"]
["","","","Pieni","dBA","28","28","28","28","29"]
["","","","Hiljainen toiminta","dBA","23","23","23","23","26"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35","6.35","6.35","6.35","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.5","9.5","9.5","9.5","9.5"]
["","Kondenssi","","","","18","18","18","18","18"]
["Ohjausjärjestelmät","Infrared remote control","","","","ARC480A11","ARC480A11","","","ARC480A11"]
["Ohjausjärjestelmät","Langallinen kaukosäädin","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Vakiovarusteet","Installation manual","","","","1","1","1","1","1"]
["","AA dry-cell batteries","","","","2","","2"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["Virransyöttö","Nimi","","","","V1","V1","V1","V1","V1"]
["","Vaihe","","","","1~","1~","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50","50","50"]
["","Jännite","","","V","220-240","220-240","220-240","220-240","220-240"]
["Vakiovarusteet","AAA dry-cell batteries","","","","","2","","2","2"]
["Ohjausjärjestelmät","Infrapuna kaukosäädin","","","","","","ARC480A11","ARC480A11"]
["Vakiovarusteet","Titanium apatite photocatalytic air purification filter","","","","","","2"]