{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A / 3AMXF-A9"]
[]
[]
[]
[]
["","","","","ATXF25A5V1B / ATXF25A5V1B / ATXF25A5V1B / 3AMXF52A2V1B9"]
["Jäähdytysteho","Min.","","kW","1.8"]
["","Nimell.","","kW","5.2"]
["","Maks.","","kW","7"]
["Lämmitysteho","Min.","","kW","1.3"]
["","Nimell.","","kW","6.8"]
["","Maks.","","kW","8"]
["Nimellinen tehokkuus","EER","","","4.05"]
["","COP","","","3.88"]
["","Vuotuinen energiankulutus","","kWh","642"]
["","Energiamerkintädirektiivi","Jäähdytys","","A"]
["","","Lämmitys","","A"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","A++"]
["","Teho","Pdesign","kW","5.2"]
["","SEER","","","7.2"]
["","Vuotuinen energiankulutus","","kWh/a","253"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","A+"]
["","Teho","Pdesign","kW","5"]
["","SCOP/A","","","4.01"]
["","Pdh Lämmitysteho -10°:ssa","","kW","3.74"]
["","Vuotuinen energiankulutus","","kWh/a","1744"]
["Energiatehokkuusalue","","","","A+++ ~ D"]