{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-G"]
[]
[]
[]
[]
["","","","","","ATXF25G5V1B","ATXF35G5V1B"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.023","0.029"]
["","Lämmitys","","Nimell.","kW","0.023","0.023"]
["Kotelo","Väri","","","","Valkoinen","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","286","286"]
["","","","Leveys","mm","770","770"]
["","","","Syvyys","mm","225","225"]
["Paino","Yksikkö","","","kg","8.5","9"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","9.8","10.9"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","8","7"]
["","","","Pieni","m³/min","6","5.7"]
["","","","Hiljainen toiminta","m³/min","4.3","4.6"]
["","","Lämmitys","Suuri","m³/min","10.4","9.3"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","8.4","7.5"]
["","","Lämmitys","Pieni","m³/min","6.4","6"]
["","","","Hiljainen toiminta","m³/min","5.3","5.2"]
["Äänen tehotaso","Jäähdytys","","","dBA","54","54"]
["","Lämmitys","","","dBA","55","56"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","40","56"]
["","","","Keski","dBA","33"]
["","","","Pieni","dBA","26"]
["","","","Hiljainen toiminta","dBA","20"]
["","Lämmitys","","Suuri","dBA","40","40"]
["","","","Keski","dBA","34","35"]
["","","","Pieni","dBA","28","29"]
["","","","Hiljainen toiminta","dBA","21","21"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6","6"]
["","Kaasu","","Ulkohalkaisija","mm","9.5","9.5"]
["","Kondenssi","","","","18","18"]
["Ohjausjärjestelmät","Infrapuna kaukosäädin","","","","ARC480A93","ARC480A93"]
["","Langallinen kaukosäädin","","","","BRC073A1","BRC073A1"]
["Vakiovarusteet","Installation manual","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Virransyöttö","Vaihe","","","","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50"]
["","Jännite","","","V","220-440","220-440"]
["Huomautukset","","","","","(1) - Jäähdytys: sisälämpötila 27°CDB, 19°CWB, ulkolämpötila 35°CDB; putkiston ekvivalenttipituus: 5m; korkeusero: 0m","(1) - Jäähdytys: sisälämpötila 27°CDB, 19°CWB, ulkolämpötila 35°CDB; putkiston ekvivalenttipituus: 5m; korkeusero: 0m"]
["","","","","","(2) - Lämmitys: sisälämpötila 20°CDB; ulkolämpötila 7°CDB, 6°CWB, kylmäaineputkiston ekvivalenttipituus: 5m (vaakasuora)","(2) - Lämmitys: sisälämpötila 20°CDB; ulkolämpötila 7°CDB, 6°CWB, kylmäaineputkiston ekvivalenttipituus: 5m (vaakasuora)"]
["","","","","","(3) - Katso sähköiset tiedot eri piirustuksista","(3) - Katso sähköiset tiedot eri piirustuksista"]