{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXL-JV"]
[]
[]
[]
[]
["","","","","ATXL25J2V1B","ATXL35J2V1B"]
["Äänenpaineen taso","Lämmitys","Suuri","dBA","41","41"]
["","","Hiljainen toiminta","dBA","26","26"]
["","","Pieni","dBA","29","29"]
["","Jäähdytys","Hiljainen toiminta","dBA","23","23"]
["","","Pieni","dBA","27","27"]
["","","Suuri","dBA","41","41"]
["","","Nimell.","dBA","35","35"]
["","Jäähdytys","Nimell.","dBA","34","34"]
["Vakiovarusteet","Asennusohje","","","1","1"]
["","Käyttöopas","","","1","1"]
["","Infrapunakauko-ohjain","","","1","1"]
["","Paristot","","","2","2"]
["","Kaukosäätimen pidike","","","1","1"]
["","Kiinnityslevy","","","1","1"]
["","Fotokatalyyttinen titaani-apatiitti-ilmanpuhdistussuodatin","","","2","2"]
["","Sisäyksikön kiinnitysruuvit","","","2","2"]
["Ohjausjärjestelmät","Infrared remote control","","","ARC433A87","ARC433A87"]
["Putkistoliitännät","Neste","Ulkohalkaisija","mm","6.35","6.35"]
["","Kaasu","Ulkohalkaisija","mm","9.5","9.5"]
["","Tyhjennys","","","18","18"]
["Ottoteho","Jäähdytys","Nimell.","kW","0.040 (2), 0.040 (3), 0.040 (4)","0.040 (2), 0.040 (3), 0.040 (4)"]
["","Lämmitys","Nimell.","kW","0.040 (2), 0.040 (3), 0.040 (4)","0.040 (2), 0.040 (3), 0.040 (4)"]
["Äänen tehotaso","Jäähdytys","","dBA","57","57"]
["","Lämmitys","","dBA","57","57"]
["Mitat","Yksikkö","Leveys","mm","770","770"]
["","","Syvyys","mm","198","198"]
["","","Korkeus","mm","283","283"]
["Kotelo","Colour","","","Valkoinen","Valkoinen"]
["Paino","Yksikkö","","kg","8","8"]
["Power supply","Vaihe","","","1~","1~"]
["","Taajuus","","Hz","50","50"]
["","Nimi","","","V1","V1"]
["","Jännite","","V","220-240","220-240"]
["Huomautukset","","","","(1) - Kytkettynä Multi-järjestelmän ulkoyksikköön, katso kytkettävän Multi-ulkoyksikön tekniset tiedot.","(1) - Kytkettynä Multi-järjestelmän ulkoyksikköön, katso kytkettävän Multi-ulkoyksikön tekniset tiedot."]
["","","","","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240 V","(4) - 240 V"]