{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R / ARXM-A8"]
[]
[]
[]
[]
["","","","","ATXM50R2V1B / ARXM50A5V1B8"]
["Jäähdytysteho","Min.","","kW","1.7"]
["","Nimell.","","kW","5"]
["","Maks.","","kW","5.3"]
["Lämmitysteho","Min.","","kW","1.7"]
["","Nimell.","","kW","5.8"]
["","Maks.","","kW","6.5"]
["Nimellinen tehokkuus","EER","","","3.45"]
["","COP","","","3.9"]
["","Vuotuinen energiankulutus","","kWh","725"]
["","Energiamerkintädirektiivi","Jäähdytys","","A"]
["","","Lämmitys","","A"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","A++"]
["","Teho","Pdesign","kW","5"]
["","SEER","","","7.4"]
["","Vuotuinen energiankulutus","","kWh/a","236"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","A++"]
["","Teho","Pdesign","kW","4.5"]
["","SCOP/A","","","4.7"]
["","Pdh Lämmitysteho -10°:ssa","","kW","4.5"]
["","Vuotuinen energiankulutus","","kWh/a","1340"]
["Huomautukset","","","","(1) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["","","","","(2) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","(3) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","(4) - Katso sähköiset tiedot eri piirustuksista"]