{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":95,"n_cols":13,"rows_kept":95,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R"]
[]
[]
[]
[]
["","","","","","ATXM20R2V1B §$ ATXM20R5V1B","ATXM20R2V1B","ATXM20R5V1B","ATXM25R2V1B","ATXM25R5V1B","ATXM35R2V1B","ATXM35R5V1B","ATXM50R2V1B"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","39"]
["","","","Keski","dBA","34"]
["","","","Hiljainen toiminta","dBA","20"]
["","","","Pieni","dBA","26"]
["","Jäähdytys","","Keski","dBA","33"]
["","","","Hiljainen toiminta","dBA","19"]
["","","","Pieni","dBA","25"]
["","","","Suuri","dBA","41"]
["Vakiovarusteet","Asennusohje","","","","1"]
["","Käyttöopas","","","","1"]
["","Langaton kaukosäädin","","","","1"]
["","AAA-kuivaparistot","","","","2"]
["","Kaukosäätimen pidike","","","","1"]
["","Kiinnityslevy","","","","1"]
["","Raikastava titaani-apatiitti-suodatin","","","","1"]
["","Sisäyksikön kiinnitysruuvit","","","","2"]
["","WLAN-sovitinsarja","","","","1"]
["Ohjausjärjestelmät","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A67"]
["Piping connections","Neste","","Ulkohalkaisija","mm","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.50"]
["","Tyhjennys","","","","18"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.029"]
["","Lämmitys","","Nimell.","kW","0.023"]
["Äänen tehotaso","Jäähdytys","","","dBA","58"]
["","Lämmitys","","","dBA","55"]
["Mitat","Yksikkö","","Leveys","mm","778"]
["","","","Syvyys","mm","272"]
["","","","Korkeus","mm","295"]
["Kotelo","Colour","","","","Valkoinen"]
["Paino","Yksikkö","","","kg","10.0"]
["Puhallin","Ilmamäärä","Lämmitys","Suuri","m³/min","9.3"]
["","","","Medium","m³/min","8.2"]
["","","","Pieni","m³/min","6.2"]
["","","","Hiljainen toiminta","m³/min","5.1"]
["","","Jäähdytys","Pieni","m³/min","5.7"]
["","","","Medium","m³/min","7.5"]
["","","","Suuri","m³/min","10.5"]
["","","","Hiljainen toiminta","m³/min","4.3"]
["Power supply","Phase","","","","1~"]
["","Nimi","","","","V1"]
["","Taajuus","","","Hz","50"]
["","Jännite","","","V","220-240"]
["Huomautukset","","","","","(1) - Jäähdytys: sisälämpötila 27°CDB, 19.0°CWB; ulkolämpötila 35°CDB, 24°CWB; putkiston ekvivalenttipituus: 5m"]
["","","","","","(2) - Lämmitys: sisälämpötila 20°CDB; ulkolämpötila 7°CDB, 6°CWB, kylmäaineputkiston ekvivalenttipituus: 5m"]
["Ottoteho","Jäähdytys","","Nimell.","kW","","0.029","0.029","0.029","0.029","0.03","0.03","0.03"]
["","Lämmitys","","Nimell.","kW","","0.023","0.023","0.022","0.022","0.027","0.027","0.032"]
["Kotelo","Väri","","","","","Valkoinen","Valkoinen","Valkoinen","Valkoinen","Valkoinen","Valkoinen","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","","295","295","295","295","295","295","299"]
["","","","Leveys","mm","","778","778","778","778","778","778","998"]
["","","","Syvyys","mm","","272","272","272","272","272","272","292"]
["Paino","Yksikkö","","","kg","","10","10","10","10","10","10","14.5"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","","10.5","10.5","10.5","10.5","11.3","11.3","15.8"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","","7.5","7.5","7.6","7.6","7.8","7.8","14"]
["","","","Pieni","m³/min","","5.7","5.7","5.7","5.7","6","6","11.4"]
["","","","Hiljainen toiminta","m³/min","","4.3","4.3","4.1","4.1","4.2","4.2","8.3"]
["","","Lämmitys","Suuri","m³/min","","9.3","9.3","9.8","9.8","9.8","9.8","15.8"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","","8.2","8.2","8","8","8.5","8.5","14.2"]
["","","Lämmitys","Pieni","m³/min","","6.2","6.2","6.3","6.3","6.5","6.5","12"]
["","","","Hiljainen toiminta","m³/min","","5.1","5.1","4.9","4.9","4.9","4.9","10.5"]
["Äänen tehotaso","Jäähdytys","","","dBA","","58","58","58","58","58","58","58"]
["","Lämmitys","","","dBA","","55","55","55","55","55","55","58"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","","41","41","41","41","45","45","44"]
["","","","Keski","dBA","","33","33","33","33","33","33","40"]
["","","","Pieni","dBA","","25","25","25","25","25","25","36"]
["","","","Hiljainen toiminta","dBA","","19","19","19","19","19","19","27"]
["","Lämmitys","","Suuri","dBA","","39","39","39","39","39","39","43"]
["","","","Keski","dBA","","34","34","34","34","35","35","39"]
["","","","Pieni","dBA","","26","26","27","27","28","28","34"]
["","","","Hiljainen toiminta","dBA","","20","20","20","20","20","20","31"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","","9.5","9.5","9.5","9.5","9.5","9.5","12.7"]
["","Kondenssi","","","","","18","18","18","18","18","18","18"]
["Ohjausjärjestelmät","Infrared remote control","","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["Ohjausjärjestelmät","Langallinen kaukosäädin","","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Vakiovarusteet","Installation manual","","","","","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","","1","1","1","1","1","1","1"]
["","Operation manual","","","","","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","1","1","1","1","1","1","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","1","1"]
["Virransyöttö","Nimi","","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Vaihe","","","","","1~","1~","1~","1~","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","","50","50","50","50","50","50","50"]
["","Jännite","","","V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Vakiovarusteet","Silver particle filter","","","","","","","","","","","1"]