{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-K3 / ARXP-K3"]
[]
[]
[]
[]
["","","","","ATXP20K3V1B / ARXP20K3V1B","ATXP25K3V1B / ARXP25K3V1B","ATXP35K3V1B / ARXP35K3V1B"]
["Jäähdytysteho","Nimell.","","kW","","2.50","3.50"]
["Nimellinen tehokkuus","EER","","","","3.79","3.45"]
["","COP","","","","4.36","4.02"]
["","Energiamerkintädirektiivi","Jäähdytys","","","A","A"]
["","","Lämmitys","","","A","A"]
["Lämmitysteho","Nimell.","","kW","","3.00","4.00"]
["Huomautukset","","","","","(1) - Jäähdytys: T2: sisälämpötila 26,6°CDB, 19,4°CWB, ulkolämpötila 48°CDB [Btu/hr/W]","(1) - Jäähdytys: T2: sisälämpötila 26,6°CDB, 19,4°CWB, ulkolämpötila 48°CDB [Btu/hr/W]"]
["","","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["","","","","","(3) - Katso sähköiset tiedot eri piirustuksista","(3) - Katso sähköiset tiedot eri piirustuksista"]
["Ulkoyksikkö","","","","ARXP20K3V1B"]
["Jäähdytysteho","Nimell.","","kW","2.00"]
["Lämmitysteho","Nimell.","","kW","2.50"]
["Nimellinen tehokkuus","EER","","","3.98"]
["","COP","","","4.77"]
["","Energiamerkintädirektiivi","Jäähdytys","","A"]
["","","Lämmitys","","A"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","A++"]
["","Teho","Pdesign","kW","2.00"]
["","SEER","","","6.75"]
["","Vuotuinen energiankulutus","","kWh/a","104"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","A++"]
["","Teho","Pdesign","kW","2.20"]
["","SCOP/A","","","4.64"]
["","Pdh Lämmitysteho -10°:ssa","","kW","2.19"]
["","Vuotuinen energiankulutus","","kWh/a","664"]