{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":81,"n_cols":8,"rows_kept":81,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-KV"]
[]
[]
[]
[]
["","","","","","ATXP20K2V1B","ATXP25K2V1B","ATXP35K2V1B"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","","40","43"]
["","","","Hiljainen toiminta","dBA","","23","26"]
["","","","Pieni","dBA","","28","29"]
["","Jäähdytys","","Hiljainen toiminta","dBA","","20","20"]
["","","","Pieni","dBA","","26","27"]
["","","","Suuri","dBA","","40","43"]
["","","","Nimell.","dBA","","34","35"]
["","Jäähdytys","","Nimell.","dBA","","33","34"]
["Vakiovarusteet","Asennusohje","","","","","1","1"]
["","Käyttöopas","","","","","1","1"]
["","Langaton kaukosäädin","","","","","1","1"]
["","AAA-kuivaparistot","","","","","2","2"]
["","Kaukosäätimen pidike","","","","","1","1"]
["","Kiinnityslevy","","","","","1","1"]
["","Fotokatalyyttinen titaani-apatiitti-ilmanpuhdistussuodatin","","","","","2","2"]
["","Sisäyksikön kiinnitysruuvit","","","","","2","2"]
["Kylmäaine","GWP","","","","","675","675"]
["Ohjausjärjestelmät","Wired remote control","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","ARC480A11","ARC480A11"]
["Putkistoliitännät","Neste","","Ulkohalkaisija","mm","","6.35","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","","9.5","9.5"]
["","Tyhjennys","","","","","18","18"]
["Sound power level","Jäähdytys","","","dBA","","55","58"]
["","Lämmitys","","","dBA","","55","58"]
["Mitat","Yksikkö","","Leveys","mm","","770","770"]
["","","","Syvyys","mm","","225","225"]
["","","","Korkeus","mm","","286","286"]
["Kotelo","Väri","","","","","Valkoinen","Valkoinen"]
["Paino","Yksikkö","","","kg","","8","8"]
["Power supply","Vaihe","","","","","1~","1~"]
["","Taajuus","","","Hz","","50","50"]
["","Nimi","","","","","V1","V1"]
["","Jännite","","","V","","220-240","220-240"]
["Huomautukset","","","","","","(1) - SL: Ilmanvirtausasetuksen hiljainen asetus puhaltimelle","(1) - SL: Ilmanvirtausasetuksen hiljainen asetus puhaltimelle"]
["Puhallin","Ilmamäärä","Jäähdytys","Nimell.","m³/min","7.8"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","33"]
["Puhallin","Ilmamäärä","Lämmitys","Nimell.","m³/min","8.5"]
["Äänenpaineen taso","Lämmitys","","Nimell.","dBA","34"]
["Kotelo","Väri","","","","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","286"]
["","","","Leveys","mm","770"]
["","","","Syvyys","mm","225"]
["Paino","Yksikkö","","","kg","8"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","9.9"]
["","","","Pieni","m³/min","5.8"]
["","","","Hiljainen toiminta","m³/min","4.8"]
["","","Lämmitys","Suuri","m³/min","10.9"]
["","","","Pieni","m³/min","6.4"]
["","","","Hiljainen toiminta","m³/min","5.2"]
["Äänen tehotaso","Jäähdytys","","","dBA","55"]
["","Lämmitys","","","dBA","55"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","39"]
["","","","Pieni","dBA","25"]
["","","","Hiljainen toiminta","dBA","20"]
["","Lämmitys","","Suuri","dBA","39"]
["","","","Pieni","dBA","28"]
["","","","Hiljainen toiminta","dBA","23"]
["Kylmäaine","GWP","","","","675"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.5"]
["","Kondenssi","","","","18"]
["Ohjausjärjestelmät","Infrapuna kaukosäädin","","","","ARC480A11"]
["","Langallinen kaukosäädin","","","","BRC944B2, BRC073A1"]
["Vakiovarusteet","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","Operation manual","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","2"]
["Virransyöttö","Nimi","","","","V1"]
["","Vaihe","","","","1~"]
["Syöttöjännite","Taajuus","","","Hz","50"]
["","Jännite","","","V","220-240"]