{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-L"]
[]
[]
[]
[]
["","","","","","ATXP20L2V1B","ATXP20L5V1B","ATXP25L2V1B","ATXP25L5V1B","ATXP35L2V1B","ATXP35L5V1B"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.017","0.017","0.019","0.019","0.032","0.032"]
["","Lämmitys","","Nimell.","kW","0.02","0.02","0.02","0.02","0.032","0.032"]
["Kotelo","Väri","","","","Valkoinen","Valkoinen","Valkoinen","Valkoinen","Valkoinen","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","286","286","286","286","286","286"]
["","","","Leveys","mm","770","770","770","770","770","770"]
["","","","Syvyys","mm","225","225","225","225","225","225"]
["Paino","Yksikkö","","","kg","9","9","9","9","9","9"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","9.8","9.8","10.1","10.1","11.5","11.5"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","7.9","7.9","8.1","8.1","8.3","8.3"]
["","","","Pieni","m³/min","5.9","5.9","6.1","6.1","6.3","6.3"]
["","","","Hiljainen toiminta","m³/min","4.4","4.4","4.4","4.4","4.5","4.5"]
["","","Lämmitys","Suuri","m³/min","10.3","10.3","10.3","10.3","11.5","11.5"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","8.4","8.4","8.6","8.6","9","9"]
["","","Lämmitys","Pieni","m³/min","6.5","6.5","6.7","6.7","7","7"]
["","","","Hiljainen toiminta","m³/min","5.3","5.3","5.3","5.3","5.3","5.3"]
["Äänen tehotaso","Jäähdytys","","","dBA","55","55","55","55","58","58"]
["","Lämmitys","","","dBA","55","55","55","55","58","58"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","39","39","40","40","43","43"]
["","","","Keski","dBA","33","33","33","33","34","34"]
["","","","Pieni","dBA","25","25","26","26","27","27"]
["","","","Hiljainen toiminta","dBA","20","20","20","20","20","20"]
["","Lämmitys","","Suuri","dBA","39","39","40","40","40","40"]
["","","","Keski","dBA","34","34","34","34","35","35"]
["","","","Pieni","dBA","28","28","28","28","29","29"]
["","","","Hiljainen toiminta","dBA","21","21","21","21","21","21"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.5","9.5","9.5","9.5","9.5","9.5"]
["","Kondenssi","","","","18","18","18","18","18","18"]
["Control systems","Infrared remote control","","","","","","ARC480A11","ARC480A11"]
["Ohjausjärjestelmät","Langallinen kaukosäädin","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Vakiovarusteet","Installation manual","","","","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2"]
["","Operation manual","","","","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1"]
["Virransyöttö","Vaihe","","","","1~","1~","1~","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50","50","50","50"]
["","Jännite","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Ohjausjärjestelmät","Infrapuna kaukosäädin","","","","ARC480A11","ARC480A11","","","ARC480A11","ARC480A11"]