{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":8,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-N9"]
[]
[]
[]
[]
["","","","","","ATXP20N5V1B9","ATXP25N5V1B9","ATXP35N5V1B9"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.019","0.020","0.032"]
["","Lämmitys","","Nimell.","kW","0.023","0.023","0.032"]
["Casing","Väri","","","","Valkoinen","Valkoinen","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","286","286","286"]
["","","","Leveys","mm","770","770","770"]
["","","","Syvyys","mm","225","225","225"]
["Paino","Yksikkö","","","kg","8.50","8.50","9.00"]
["Fan","Ilmamäärä","Jäähdytys","Suuri","m³/min","9.5","9.7","11.5"]
["","","","Medium","m³/min","7.4","7.7","8.3"]
["","","","Pieni","m³/min","5.6","5.8","6.3"]
["","","","Hiljainen toiminta","m³/min","4.2","4.2","4.5"]
["","","Lämmitys","Suuri","m³/min","10.4","10.4","11.5"]
["","","","Medium","m³/min","8.1","8.1","9.0"]
["","","","Pieni","m³/min","6.2","6.4","7.0"]
["","","","Hiljainen toiminta","m³/min","5.2","5.2","5.1"]
["Äänen tehotaso","Jäähdytys","","","dBA","55","55","58"]
["","Lämmitys","","","dBA","55","55","58"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","39","40","43"]
["","","","Medium","dBA","33","33","34"]
["","","","Pieni","dBA","25","26","27"]
["","","","Hiljainen toiminta","dBA","19","19","20"]
["","Lämmitys","","Suuri","dBA","39","40","40"]
["","","","Keski","dBA","34","34","35"]
["","","","Pieni","dBA","28","28","29"]
["","","","Hiljainen toiminta","dBA","21","21","21"]
["Piping connections","Liquid","","Ulkohalkaisija","mm","6","6","6"]
["","Gas","","Ulkohalkaisija","mm","9.50","9.50","9.50"]
["","Tyhjennys","","","","18","18","18"]
["Control systems","Infrared remote control","","","","ARC480A78","ARC480A78","ARC480A78"]
["","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1"]
["Vakiovarusteet","Asennusohje","","","","1","1","1"]
["","Käyttöopas","","","","1","1","1"]
["","Infrapunakauko-ohjain","","","","1","1","1"]
["","AAA-kuivaparistot","","","","2","2","2"]
["","Kaukosäätimen pidike","","","","1","1","1"]
["","Kiinnityslevy","","","","1","1","1"]
["","Raikastava titaani-apatiitti-suodatin","","","","1","1","1"]
["","Hopeahiukkassuodatin","","","","1","1","1"]
["","Sisäyksikön kiinnitysruuvit","","","","2","2","2"]
["","Yleiset varotoimet","","","","1","1","1"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Taajuus","","","Hz","50","50","50"]
["","Jännite","","","V","220-240","220-240","220-240"]
["Huomautukset","","","","","(1) - Jäähdytys: sisälämpötila 27°CDB, 19°CWB, ulkolämpötila 35°CDB; putkiston ekvivalenttipituus: 5m; korkeusero: 0m","(1) - Jäähdytys: sisälämpötila 27°CDB, 19°CWB, ulkolämpötila 35°CDB; putkiston ekvivalenttipituus: 5m; korkeusero: 0m","(1) - Jäähdytys: sisälämpötila 27°CDB, 19°CWB, ulkolämpötila 35°CDB; putkiston ekvivalenttipituus: 5m; korkeusero: 0m"]
["","","","","","(2) - Lämmitys: sisälämpötila 20°CDB; ulkolämpötila 7°CDB, 6°CWB, kylmäaineputkiston ekvivalenttipituus: 5m (vaakasuora)","(2) - Lämmitys: sisälämpötila 20°CDB; ulkolämpötila 7°CDB, 6°CWB, kylmäaineputkiston ekvivalenttipituus: 5m (vaakasuora)","(2) - Lämmitys: sisälämpötila 20°CDB; ulkolämpötila 7°CDB, 6°CWB, kylmäaineputkiston ekvivalenttipituus: 5m (vaakasuora)"]
["","","","","","(3) - Katso sähköiset tiedot eri piirustuksista","(3) - Katso sähköiset tiedot eri piirustuksista","(3) - Katso sähköiset tiedot eri piirustuksista"]