{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":8,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZAS-MY1"]
[]
[]
[]
[]
["","","","","","AZAS100M7Y1B","AZAS125M7Y1B","AZAS140M7Y1B"]
["Mitat","Yksikkö","","Korkeus","mm","990","990","990"]
["","","","Leveys","mm","940","940","940"]
["","","","Syvyys","mm","320","320","320"]
["Paino","Unit","","","kg","","70"]
["Kompressori","Tyyppi","","","","","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-5","-5","-5"]
["","","","Maks.","°CDB","46","46","46"]
["","Lämmitys","Ympäristö","Min.","°CWB","-15","-15","-15"]
["","","","Maks.","°CWB","15.5","15.5","15.5"]
["Äänen tehotaso","Jäähdytys","","","dBA","70","71","73"]
["","Lämmitys","","","dBA","","71","73 (1)"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","53","53","54"]
["","Lämmitys","","Nimell.","dBA","57","57","57"]
["Kylmäaine","Tyyppi","","","","R-32","R-32","R-32"]
["","Täytösmäärä","","","kg","2.60","2.60","2.90"]
["Kylmäaine","GWP","","","","","675"]
["Kylmäaine","Täytösmäärä","","","tCO2Eq","1.76","1.76","1.96"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","9.52","9.52","9.52"]
["Putkiliitännät","Kaasu","","Ulkohalkaisija","mm","","15.9"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","30","30","30"]
["","","Järjestelmä","Ekvivalentti","m","50","50","50"]
["","","","Täyttämätön","m","30","30","30"]
["","Lisäkylmäainemäärä","","","kg/m","Katso asennusohje","Katso asennusohje","Katso asennusohje"]
["","Korkeusero","IU - OU","Maks.","m","30.0","30.0","30.0"]
["","","IU - IU","Maks.","m","0.5","0.5","0.5"]
["Vakiovarusteet","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Virransyöttö","Vaihe","","","","3~","3~","3~"]
["Syöttöjännite","Syöttöjännite-=-Taajuus","","Taajuus","","50","50","50"]
["","Syöttöjännite-=-Jännite","","Jännite","","380-415","380-415","380-415"]
["Virta - 50&nbsp;Hz","Virta - 50&nbsp;Hz-=-Varokkeiden enimmäisvirta (MFA)","","Virta - 50&nbsp;Hz-=-Varokkeiden enimmäisvirta (MFA)-=-A","","","16"]
["Huomautukset","","","","","","(1) - ENER Lot 21 mukaisesti","(1) - ENER Lot 21 mukaisesti"]
["Paino","Yksikkö","","","kg","70","","77"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori","","Hermeettisesti suljettu swing-kompressori"]
["Kylmäaine","GWP","","","","675","","675"]
["Putkiliitännät","Kaasu","","Ulkohalkaisija","mm","15.9","","15.9"]
["Virta - 50&nbsp;Hz","Virta - 50&nbsp;Hz-=-Sulakkeiden enimmäisvirta (MFA)-=-A","","","A","16","","16"]