{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDK"]
[]
[]
[]
[]
["","","","","BRC1HHDAK (Archived)","BRC1HHDAKA (Archived)"]
["Kotelo","Väri","","","Musta","Musta"]
["","Painikesuojus","","","Ei","Ei"]
["","Toiminnan LED","Väri","","Sininen tilamerkkivalo","Sininen tilamerkkivalo"]
["Mitat","Yksikkö","Korkeus","mm","85","85"]
["","","Leveys","mm","85","85"]
["","","Syvyys","mm","25","25"]
["","Pakattu yksikkö","Korkeus","mm","50","50"]
["","","Leveys","mm","217","217"]
["","","Syvyys","mm","161","161"]
["Paino","Yksikkö","","kg","0.110","0.110"]
["","Pakattu yksikkö","","kg","0.317","0.317"]
["Pakkaus","Materiaali","","","Kartonki","Kartonki"]
["","Paino","","kg","0.0850","0.0850"]
["LCD","Tyyppi","","","100 x 150 pistettä","100 x 150 pistettä"]
["","Mitat","Korkeus","mm","40.7","40.7"]
["","","Leveys","mm","28.0","28.0"]
["","Taustavalo","Väri","","Valkoinen","Valkoinen"]
["Ympäristön lämpötila","Toiminta","Min.","°C","-10","-10"]
["","","Maks.","°C","50","50"]
["","Säilytys","Min.","°C","-20","-20"]
["","","Maks.","°C","70","70"]
["","Ympäristön lämpötila-=-Suhteellinen kosteus <-=-%","","%","95","95"]
["Ohjausjärjestelmät","Lämpötilan ohjauksen luokka","","","VI","VI"]
["","Vaikutus kausittaiseen tilojen lämmityksen tehokkuuteen","","%","4.0","4.0"]
["Johtoliitännät","Johdotuksen pituus","Enint.","m","500","500"]