{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":12,"n_cols":7,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 3MXM-A8"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32 / 3MXM52A2V1B8","CHYHBH05AAV32 / 3MXM68A2V1B8"]
["Lämmitysteho","Nimell.","","","kW","4.41","4.50"]
["COP","","","","","4.49","3.91"]
["Lämminvesivaraaja","Yleistä","","Ilmoitettu kuormitusprofiili","","XL","XL"]
["","Keskimääräinen ilmasto","","Vedenlämmityksen energiatehokkuusluokka","","A","A"]
["Tilojen lämmitys","Keskimäär. ilmaston veden lähtö 55 °C","Yleistä","SCOP","","2.86","2.91"]
["","","","Kausittainen tilojen lämmityksen tehokk.luokka","","A+","A+"]