{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AT"]
[]
[]
[]
[]
["","","","","CTXA15A2V1BT"]
["Äänenpaineen taso","Lämmitys","Suuri","dBA","39"]
["","","Keski","dBA","32"]
["","","Hiljainen toiminta","dBA","21"]
["","","Pieni","dBA","25"]
["","Jäähdytys","Keski","dBA","32"]
["","","Hiljainen toiminta","dBA","21"]
["","","Pieni","dBA","25"]
["","","Suuri","dBA","39"]
["Vakiovarusteet","Asennusohje","","","1"]
["","Käyttöopas","","","1"]
["","Ilmansuodatin","","","2"]
["","Infrapunakauko-ohjain","","","1"]
["","Kaukosäätimen kiinnityslevy","","","1"]
["","Ruuvipussi","","","1"]
["","Ruuvinsuoja","","","1"]
["","AAA-kuivaparistot","","","2"]
["","Yleiset varotoimet","","","1"]
["Kylmäaine","GWP","","","675.0"]
["Control systems","Wired remote control","","","BRC073"]
["","Infrared remote control","","","ARC466A58"]
["Putkiliitännät","Neste","Ulkohalkaisija","mm","6.35"]
["","Kaasu","Ulkohalkaisija","mm","9.50"]
["","Kondenssi","","","18"]
["Ottoteho","Jäähdytys","Nimell.","kW","0.020"]
["","Lämmitys","Nimell.","kW","0.020"]
["Äänen tehotaso","Jäähdytys","","dBA","57"]
["Mitat","Yksikkö","Leveys","mm","798"]
["","","Syvyys","mm","189"]
["","","Korkeus","mm","295"]
["Kotelo","Colour","","","Mustapuu"]
["Paino","Yksikkö","","kg","12"]
["Power supply","Phase","","","1~"]
["","Taajuus","","Hz","50"]
["","Nimi","","","V1"]
["","Jännite","","V","220-240"]