{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-CB"]
[]
[]
[]
[]
["","","","","","CTXA15C2V1BB"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.020"]
["","Lämmitys","","Nimell.","kW","0.020"]
["Casing","Väri","","","","Musta"]
["Mitat","Yksikkö","","Korkeus","mm","295"]
["","","","Leveys","mm","798"]
["","","","Syvyys","mm","189"]
["Paino","Yksikkö","","","kg","11.5"]
["Fan","Ilmamäärä","Jäähdytys","Suuri","m³/min","11.0"]
["","","","Medium","m³/min","8.2"]
["","","","Pieni","m³/min","6.1"]
["","","","Hiljainen toiminta","m³/min","4.6"]
["","","Lämmitys","Suuri","m³/min","10.9"]
["","","","Medium","m³/min","8.7"]
["","","","Pieni","m³/min","6.4"]
["","","","Hiljainen toiminta","m³/min","4.5"]
["Äänen tehotaso","Jäähdytys","","","dBA","57"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","39"]
["","","","Medium","dBA","32"]
["","","","Pieni","dBA","25"]
["","","","Hiljainen toiminta","dBA","21"]
["","Lämmitys","","Suuri","dBA","39"]
["","","","Keski","dBA","32"]
["","","","Pieni","dBA","25"]
["","","","Hiljainen toiminta","dBA","21"]
["Kylmäaine","GWP","","","","675.0"]
["Piping connections","Liquid","","Ulkohalkaisija","mm","6.35"]
["","Gas","","Ulkohalkaisija","mm","9.50"]
["","Tyhjennys","","","","18"]
["Control systems","Infrared remote control","","","","ARC466A85"]
["","Wired remote control","","","","BRC073A1"]
["Vakiovarusteet","Asennusohje","","","","1"]
["","Käyttöopas","","","","1"]
["","Ilmansuodatin","","","","2"]
["","Infrapunakauko-ohjain","","","","1"]
["","Kaukosäätimen kiinnityslevy","","","","1"]
["","Ruuvipussi","","","","1"]
["","Ruuvinsuoja","","","","2"]
["","AAA-kuivaparistot","","","","2"]
["","Yleiset varotoimet","","","","1"]
["Power supply","Name","","","","V1"]
["","Phase","","","","1~"]
["","Taajuus","","","Hz","50"]
["","Jännite","","","V","220-240"]