{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":7,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-M / 2MXM-M"]
[]
[]
[]
[]
["","","","","CTXM15M2V1B / CTXM15M2V1B / 2MXM40M2V1B","CTXM15M2V1B / CTXM15M2V1B / 2MXM40M3V1B","CTXM15M2V1B / CTXM15M2V1B / 2MXM50M2V1B"]
["Jäähdytysteho","Nimell.","","kW","3.00","3.0","3.00"]
["Nimellinen tehokkuus","Annual energy consumption","","kWh","302 (0.000)","302","310"]
["","EER","","","4.97","4.97","4.84"]
["","COP","","","4.35","4.35","4.58"]
["","Energiamerkintädirektiivi","Jäähdytys","","A","A","A"]
["","","Lämmitys","","A","A","A"]
["Lämmitysteho","Nimell.","","kW","3.50","3.50"]
["Huomautukset","","","","","(1) - Nimelliset jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m. Vakiotehokkuussarjan tiedot"]
["","","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["Lämmitysteho","Min.","","kW","","","4.00"]
["Huomautukset","","","","","","(1) - EER/COP Eurovent 2012 -standardin mukaan, käytettäväksi ainoastaan EU:n ulkopuolella"]