{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CVXM-A9"]
[]
[]
[]
[]
["","","","","","CVXM20A3V1B9"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.02"]
["","Lämmitys","","Nimell.","kW","0.02"]
["Kotelo","Väri","","","","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","600"]
["","","","Leveys","mm","750"]
["","","","Syvyys","mm","238"]
["Paino","Yksikkö","","","kg","17"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","8.7"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","7"]
["","","","Pieni","m³/min","4.9"]
["","","","Hiljainen toiminta","m³/min","4.1"]
["","","Lämmitys","Suuri","m³/min","9.2"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","7.2"]
["","","Lämmitys","Pieni","m³/min","5.6"]
["","","","Hiljainen toiminta","m³/min","4.1"]
["Äänen tehotaso","Jäähdytys","","","dBA","52"]
["","Lämmitys","","","dBA","52"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","38"]
["","","","Keski","dBA","32"]
["","","","Pieni","dBA","25"]
["","","","Hiljainen toiminta","dBA","22"]
["","Lämmitys","","Suuri","dBA","38"]
["","","","Keski","dBA","32"]
["","","","Pieni","dBA","25"]
["","","","Hiljainen toiminta","dBA","21"]
["Kylmäaine","GWP","","","","675"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.4"]
["","Kaasu","","Ulkohalkaisija","mm","9.5"]
["","Kondenssi","","","","VP20 (I.D. 20/O.D. 26)"]
["Control systems","Infrared remote control","","","","ARC466A66"]
["Ohjausjärjestelmät","Langallinen kaukosäädin","","","","BRC073A1"]
["Vakiovarusteet","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Virransyöttö","Vaihe","","","","1~"]
["Syöttöjännite","Taajuus","","","Hz","50"]
["","Jännite","","","V","220-240"]