{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":9,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2U30GC-A"]
[]
[]
[]
[]
["","","","","","D2U30GC015AB","D2U30GC020AB","D2U30GC015AA (Archived)","D2U30GC020AA (Archived)"]
["Lämpöhäviöt","Boilerin valmiustila Ps","","","kW","0.0","0.0"]
["","Boilerin valmiustila","","","kWh / 24h","","","1.5","1.5"]
["","Boilerin valmiustila qS","","","kW","0.0","0.0"]
["Kuuma käyttövesi","Lämmöntuonti (bruttolämpöarvo) Qnw","Nim.","Maksimi","kW","16.7","22.2","16.7","22.2"]
["","","","Minimi","kW","3.3","3.3","3.3","3.3"]
["","Teho","","Minimi","kW","3.0","3.0","3.0","3.0"]
["","Lämpötila","","Maksimi","°C","70","70","85","85"]
["","Lämmöntuonti (nettolämpöarvo) Qnw","Nim.","Minimi","kW","3.0","3.0","3.0","3.0"]
["","","","Maksimi","kW","15.0","20.0","15.0","20.0"]
["","Tehokkuus","","NL-ominaisuudet (DIN4708)","","2.0","2.1","2.0","2.1"]
["Palokaasu","Lämpötila","","Maksimi","°C","63","69","63","69"]
["","Massavirtaus (G31)","","Maksimi","kg/h","22.5","30.0","22.5","30.0"]
["Puhallusilma","Samankeskinen","","","","Kyllä","Kyllä","Kyllä","Kyllä"]
["Lämminvesivaraaja","Yleistä","","Vedenlämmityksen energiatehokkuusluokka","","A","A","A","A"]
["","","","Ilmoitettu kuormitusprofiili","","L","L","L","L"]
["Mitat","Yksikkö","Korkeus","Kotelo","mm","1,895","1,895","1,895","1,895"]
["Kotelo","Väri","","","","Liike valkoinen (RAL9016) / tummanharmaa (RAL7011)","Liike valkoinen (RAL9016) / tummanharmaa (RAL7011)","Liike valkoinen (RAL9016) / tummanharmaa (RAL7011)","Liike valkoinen (RAL9016) / tummanharmaa (RAL7011)"]
["Säiliö","Materiaali","","","","Polypropyleeni","Polypropyleeni","Polypropyleeni","Polypropyleeni"]
["Tilojen lämmitys","Yleistä","","Kausittainen tilojen lämmityksen tehokk.luokka","","A","A","A","A"]
["","","","ηs (kausittainen tilojen lämmityksen tehokkuus)","%","91","92","91","92"]
["Keskuslämmitys","Lämmöntuonti Qn (bruttolämpöarvo)","Nim.","Minimi","kW","3.3","3.3","3.3","3.3"]
["","","","Maksimi","kW","16.7","22.2","16.7","22.2"]
["","Veden lämpötila","","Maksimi","°C","85","85","90","90"]
["","Teho Pn, 80/60°C","","Minimi","kW","2.9","2.9","2.9","2.9"]
["","","","Nim.","kW","14.6","19.5","14.6","19.5"]
["","Lämmöntuonti Qn (nettolämpöarvo)","Nim.","Maksimi","kW","15.0","20.0","15.0","20.0"]
["","","","Minimi","kW","3.0","3.0","3.0","3.0"]
["","Teho Pnc, 50/30°C","","Minimi","kW","3.2","3.2","3.2","3.2"]
["","","","Nim.","kW","15.7","20.9","15.7","20.9"]
["Kaasu","Liitäntä","","Halkaisija","mm","20","20","20","20"]
["","Kulutus (G31)","","Minimi","m³/h","0.16","0.16","0.16","0.16"]
["","","","Maksimi","m³/h","0.62","0.82","0.62","0.82"]
["","NOx-luokka","","","","6","6","6","6"]
["Huomautukset","","","","","(1) - Lämpöhäviöt EN12897 mukaan","(1) - Lämpöhäviöt EN12897 mukaan"]