{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Ottoteho","kW","","","","0.015"]
["Kytkettävien sisäyksiköiden enimmäismäärä","","","","","32"]
["Kytkettävien ulkoyksiköiden enimmäismäärä @","","","","","7"]
["Mitat","Yksikkö","","Korkeus","mm","136"]
["","","","Leveys","mm","384"]
["","","","Syvyys","mm","92"]
["Tiedonsiirto","DIII-NET","","Määrä","","1"]
["","","","Huomautus","","DIII-NET (F1F2)"]
["","Ethernet","","Määrä","","1"]
["","Tuloliitin","Digitaalinen","Määrä","","4"]
["Ympäristön lämpötila","Toiminta","","Min.","°C","-10"]
["","","","Maks.","°C","50"]
["","Säilytys","","Min.","°C","-20"]
["","","","Maks.","°C","60"]
["","Ympäristön lämpötila-=-Suhteellinen kosteus <-=-%","","","%","85"]
["Syöttöjännite","Taajuus","","","Hz","50/60"]
["","Jännite","","","V","110-240 AC"]
["Huomautukset","","","","","(1) - Sisältää WAGO-virtalähteen ottotehon, CPU-moduulin ja I/O-moduulin"]
["","","","","","(2) - Mittoihin kuuluvat WAGO-virtalähde, CPU-moduuli, I/O-moduuli ja eri osien välillä tarvittava tila"]
["","","","","","(3) - Valinnaisen näytön mittasuhteet ovat: korkeus: 209mm, leveys: 123mm, syvyys: 8,5mm"]