{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Ympäristön lämpötila","Suhteellinen kosteus <","","","%","85"]
["Kytkettävien sisäyksiköiden enimmäismäärä","","","","","32"]
["Ottoteho","kW","","","","0.015 (1)"]
["Tiedonsiirto","DIII-NET","","Määrä","","1"]
["","","","Huomautus","","DIII-NET (F1F2)"]
["","Ethernet","","Määrä","","1"]
["","Tuloliitin","Digitaalinen","Määrä","","4"]
["Mitat","Yksikkö","","Leveys","mm","384"]
["","","","Syvyys","mm","92"]
["","","","Korkeus","mm","136"]
["Kytkettävien ulkoyksiköiden enimmäismäärä","","","","","7"]
["Power supply","Taajuus","","","Hz","50/60"]
["","Jännite","","","V","110-240 AC"]
["Huomautukset","","","","","(1) - Sisältää WAGO-virtalähteen ottotehon, CPU-moduulin ja I/O-moduulin"]
["","","","","","(2) - Mittoihin kuuluvat WAGO-virtalähde, CPU-moduuli, I/O-moduuli ja eri osien välillä tarvittava tila"]
["","","","","","(3) - Valinnaisen näytön mittasuhteet ovat: korkeus: 209mm, leveys: 123mm, syvyys: 8,5mm"]