{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EABX-D6V7 / EPGA011-016DV7"]
[]
[]
[]
[]
["","","","","","EABX16DF6V7 / EPGA11DAV37","EABX16DF6V7 / EPGA14DAV37","EABX16DF6V7 / EPGA16DAV37"]
["COP","","","","","5.15 (1), 3.88 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)"]
["Sisäyksikkö","","","","","EABX16DA6V7","EABX16DA6V7","EABX16DA6V7"]
["Tilojen lämmitys","Keskimäär. ilmaston veden lähtö 55 °C","Yleistä","Seasonal space heating eff. class","","","A++"]
["","","","ηs (kausittainen tilojen lämmityksen tehokkuus)","%","","132"]
["","","","SCOP","","","3.37"]
["Jäähdytysteho","Nimell.","","","kW","","11.1 (1), 11.9 (2)"]
["EER","","","","","4.75 (1), 3.23 (2)","4.09 (1), 2.99 (2)","3.94 (1), 2.99 (2)"]
["Lämmitysteho","Nimell.","","","kW","","14.5 (1), 14.5 (2)"]
["Ottoteho","Jäähdytys","","Nimell.","kW","","2.72 (1), 3.97 (2)"]
["","Lämmitys","","Nimell.","kW","","2.91 (1), 3.96 (2)"]
["Huomautukset","","","","","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["Lämmitysteho","Nimell.","","","kW","11.1 (1), 11.3 (2)","","16.5 (1), 15.6 (2)"]
["Jäähdytysteho","Nimell.","","","kW","10.5 (1), 10.7 (2)","","13.5 (1), 11.9 (2)"]
["Ottoteho","Lämmitys","","Nimell.","kW","2.16 (1), 2.91 (2)","","3.45 (1), 4.21 (2)"]
["","Jäähdytys","","Nimell.","kW","2.21 (1), 3.30 (2)","","3.42 (1), 3.97 (2)"]
["Tilojen lämmitys","Keskimäär. ilmaston veden lähtö 55 °C","Yleistä","SCOP","","3.32","","3.43"]
["","","","Kausittainen tilojen lämmityksen tehokk.luokka","","A++","","A++"]
["","Keskimäär. ilmaston veden lähtö 35°C","Yleistä","SCOP","","4.44","","4.61"]
["","","","Kausittainen tilojen lämmityksen tehokk.luokka","","A+++","","A+++"]
["Energiatehokkuusalue","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]