{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":17,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EAVH-D6V7 / EPGA011-016DV7"]
[]
[]
[]
[]
["","","","","","EAVH16S18DA6V7 / EPGA11DAV37","EAVH16S23DA6V7 / EPGA11DAV37","EAVH16S18DJ6V7 / EPGA11DAV37","EAVH16S23DJ6V7 / EPGA11DAV37","EAVH16S18DJ6V7 / EPGA14DAV37","EAVH16S23DJ6V7 / EPGA14DAV37","EAVH16S18DA6V7 / EPGA14DAV37","EAVH16S23DA6V7 / EPGA14DAV37","EAVH16S18DJ6V7 / EPGA16DAV37","EAVH16S23DJ6V7 / EPGA16DAV37","EAVH16S18DA6V7 / EPGA16DAV37","EAVH16S23DA6V7 / EPGA16DAV37"]
["Lämminvesivaraaja","Yleistä","","Ilmoitettu kuormitusprofiili","","L","XL","L","XL","L","XL","L","XL","L","XL","L","XL"]
["","Keskimääräinen ilmasto","","Vedenlämmityksen energiatehokkuusluokka","","A","A","A","A","A","A","A","A","A","A","A","A"]
["COP","","","","","5.15 (1), 3.88 (2)","5.15 (1), 3.88 (2)","5.15 (1), 3.88 (2)","5.15 (1), 3.88 (2)","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)"]
["Sisäyksikkö","","","","","EAVH16S18DA6V7","EAVH16S23DA6V7","EAVH16S18DJ6V7","EAVH16S23DJ6V7","EAVH16S18DJ6V7","EAVH16S23DJ6V7","EAVH16S18DA6V7","EAVH16S23DA6V7","EAVH16S18DJ6V7","EAVH16S23DJ6V7","EAVH16S18DA6V7","EAVH16S23DA6V7"]
["Tilojen lämmitys","Keskimäär. ilmaston veden lähtö 55 °C","Yleistä","Seasonal space heating eff. class","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","","","ηs (kausittainen tilojen lämmityksen tehokkuus)","%","129","129","129","129","130","130","130","130","133","133","133","133"]
["","","","SCOP","","3.29","3.29","3.29","3.29","3.34","3.34","3.34","3.34","3.41","3.41","3.41","3.41"]
["Lämpenemisaika 10°C...50 °C","hr","","","","53min at 7°C ambient temperature","1h02min at 7°C ambient temperature","53min at 7°C ambient temperature","1h02min at 7°C ambient temperature","53min at 7°C ambient temperature","1h02min at 7°C ambient temperature","53min at 7°C ambient temperature","1h02min at 7°C ambient temperature","53min at 7°C ambient temperature","1h02min at 7°C ambient temperature","53min at 7°C ambient temperature","1h02min at 7°C ambient temperature"]
["Lämmitysteho","Nimell.","","","kW","11.1 (1), 11.3 (2)","11.1 (1), 11.3 (2)","11.1 (1), 11.3 (2)","11.1 (1), 11.3 (2)","14.5 (1), 14.5 (2)","14.5 (1), 14.5 (2)","14.5 (1), 14.5 (2)","14.5 (1), 14.5 (2)","16.5 (1), 15.6 (2)","16.5 (1), 15.6 (2)","16.5 (1), 15.6 (2)","16.5 (1), 15.6 (2)"]
["Ottoteho","Lämmitys","","Nimell.","kW","2.16 (1), 2.91 (2)","2.16 (1), 2.91 (2)","2.16 (1), 2.91 (2)","2.16 (1), 2.91 (2)","2.91 (1), 3.96 (2)","2.91 (1), 3.96 (2)","2.91 (1), 3.96 (2)","2.91 (1), 3.96 (2)","3.45 (1), 4.21 (2)","3.45 (1), 4.21 (2)","3.45 (1), 4.21 (2)","3.45 (1), 4.21 (2)"]
["","Kuuma käyttövesi 10°C...50 °C","","Nim.","kWh","2.67","3.08","2.67","3.08","2.67","3.08","2.67","3.08","2.67","3.08","2.67","3.08"]
["Huomautukset","","","","","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]