{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSH-D"]
[]
[]
[]
[]
["","","","","","EBSH11P30DF","EBSH11P50DF","EBSH11P30DG","EBSH11P50DG","EBSH16P30DF","EBSH16P50DF","EBSH16P30DG","EBSH16P50DG"]
["Kotelo","Väri","","","","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)"]
["","Materiaali","","","","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni"]
["Mitat","Yksikkö","","Korkeus","mm","1,893","1,910","1,893","1,910","1,893","1,910","1,893","1,910"]
["","","","Leveys","mm","594","792","594","792","594","792","594","792"]
["","","","Syvyys","mm","680","817","680","817","680","817","680","817"]
["Paino","Yksikkö","","","kg","93","114","93","114","93","114","93","114"]
["PED","Luokka","","","","Luokka II","Luokka II","Luokka II","Luokka II","Luokka II","Luokka II","Luokka II","Luokka II"]
["Kylmäaine","Tyyppi","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["","Täytösmäärä","","","kg","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80"]
["","Täytösmäärä","","","tCO2Eq","2.57","2.57","2.57","2.57","2.57","2.57","2.57","2.57"]
["Äänen tehotaso","Nimell.","","","dBA","44.7","44.7","44.7","44.7","49.0","49.0","49.0","49.0"]
["Äänenpaineen taso","Nimell.","","","dBA","36.8","36.8","36.8","36.8","40.3","40.3","40.3","40.3"]
["Toimintalämpötila-alue","Lämmitys","Vesi","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Maks.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","Jäähdytys","Ympäristö","Min.","°CDB","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","Vesi","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Maks.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["Virransyöttö","Vaihe","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50","50","50","50","50","50"]
["","Jännite","","","V","230","230","230","230","230","230","230","230"]
["Huomautukset","","","","","(1) - Lämpöhäviöt EN12897 mukaan","(1) - Lämpöhäviöt EN12897 mukaan","(1) - Lämpöhäviöt EN12897 mukaan","(1) - Lämpöhäviöt EN12897 mukaan","(1) - Lämpöhäviöt EN12897 mukaan","(1) - Lämpöhäviöt EN12897 mukaan","(1) - Lämpöhäviöt EN12897 mukaan","(1) - Lämpöhäviöt EN12897 mukaan"]
["","","","","","(2) - Katso toimintarajojen piirros","(2) - Katso toimintarajojen piirros","(2) - Katso toimintarajojen piirros","(2) - Katso toimintarajojen piirros","(2) - Katso toimintarajojen piirros","(2) - Katso toimintarajojen piirros","(2) - Katso toimintarajojen piirros","(2) - Katso toimintarajojen piirros"]