{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":13,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSXB-D / ERLA-DW17"]
[]
[]
[]
[]
["","","","","","EBSXB16P30DF / ERLA16D2W17","EBSXB16P50DF / ERLA16D2W17","EBSXB16P30DF / ERLA16DAW17","EBSXB16P50DF / ERLA16DAW17","EBSXB16P50DG / ERLA16D2W17","EBSXB16P30DG / ERLA16DAW17","EBSXB16P30DG / ERLA16D2W17","EBSXB16P50DG / ERLA16DAW17"]
["Sisäyksikkö","","","","","EBSXB16P30DF","EBSXB16P50DF","EBSXB16P30DF","EBSXB16P50DF","EBSXB16P50DG","EBSXB16P30DG","EBSXB16P30DG","EBSXB16P50DG"]
["Lämmitysteho","Nimell.","","","kW","16.0 (1)","16.0 (1)","16.0 (1)","16.0 (1)","16.0","16.0","16.0","16.0"]
["Jäähdytysteho","Nimell.","","","kW","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)"]
["Ottoteho","Lämmitys","","Nimell.","kW","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)"]
["","Jäähdytys","","Nimell.","kW","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)"]
["COP","","","","","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)"]
["EER","","","","","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)"]
["Lämminvesivaraaja","Yleistä","","Ilmoitettu kuormitusprofiili","","L","XL","L","XL","XL","L","L","XL"]
["","Keskimääräinen ilmasto","","Vedenlämmityksen energiatehokkuusluokka","","A+","A+","A+","A+","A+","A+","A+","A+"]
["Tilojen lämmitys","Keskimäär. ilmaston veden lähtö 55 °C","Yleistä","SCOP","","3.35","3.35","3.35","3.35","3.35","3.35","3.35","3.35"]
["","","","Kausittainen tilojen lämmityksen tehokk.luokka","","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Keskimäär. ilmaston veden lähtö 35°C","Yleistä","SCOP","","4.68","4.68","4.68","4.68","4.68","4.68","4.68","4.68"]
["","","","Kausittainen tilojen lämmityksen tehokk.luokka","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Energiatehokkuusalue","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Huomautukset","","","","","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]