{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSAX-D9W"]
[]
[]
[]
[]
["","","","","","EGSAX06DA9W","EGSAX10DA9W"]
["Lämmitysteho","Min.","","","kW","0.85","0.85"]
["","Nimell.","","","kW","3.35","5.49"]
["","Maks.","","","kW","7.98","9.55"]
["Ottoteho","Nim.","","","kW","0.74","1.17"]
["COP","","","","","4.51","4.70"]
["Kotelo","Colour","","","","Valkoinen + Musta","Valkoinen + Musta"]
["","Materiaali","","","","Pinnoitettu metallilevy"]
["Mitat","Yksikkö","","Korkeus","mm","1,891","1,891"]
["","","","Leveys","mm","597","597"]
["","","","Syvyys","mm","666","666"]
["Paino","Yksikkö","","","kg","222","222"]
["Säiliö","Vesitilavuus","","","l","180"]
["","Eristys","","Lämpöhäviö","kWh / 24 h","1.2","1.2"]
["","Korroosionsuojaus","","","","Peittaus","Peittaus"]
["Kylmäaine","Tyyppi","","","","R-32","R-32"]
["","GWP","","","","675.0","675.0"]
["","Täytösmäärä","","","kg","1.70","1.70"]
["Toimintalämpötila-alue","Asennustila","","Min.","°C","5","5"]
["","","","Maks.","°C","35","35"]
["","Suolavesipuoli","","Min.","°C","-10","-10"]
["","","","Maks.","°C","30","30"]
["","Heating","Vesi","Min.","°C","5","5"]
["","","","Maks.","°C","65","65"]
["","Kuuma käyttövesi","Vesi","Min.","°C","25","25"]
["","","","Maks.","°C","60","60"]
["Tilojen lämmitys","Keskimäär. ilmaston veden lähtö 55 °C","Yleistä","SCOP","","3.77 (1)","4.05 (1)"]
["","","","Seasonal space heating eff. class","","A++","A+++"]
["","Keskimäär. ilmaston veden lähtö 35°C","Yleistä","SCOP","","5.18 (1)","5.20 (1)"]
["","","","Kausittainen tilojen lämmityksen tehokk.luokka","","A+++","A+++"]
["Power supply","Phase","","","","1~/3~","1~/3~"]
["","Taajuus","","","Hz","50","50"]
["","Jännite","","","V","230/400","230/400"]
["Virta","Suositeltu sulakekoko","","","A","16/32","16/32"]
["Huomautukset","","","","","(1) - Standardien EN14825 ja EN14511 mukaisesti:2018","(1) - Standardien EN14825 ja EN14511 mukaisesti:2018"]
["","","","","","(2) - Katso toimintalämpötila-alue-piirros: alueen lisäys lisä- tai varalämmittimellä","(2) - Katso toimintalämpötila-alue-piirros: alueen lisäys lisä- tai varalämmittimellä"]