{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Äänenpaineen taso","Nimell.","","","dBA","32.0 (6)"]
["Kylmäaine","GWP","","","","2,090"]
["","Täytösmäärä","","","kg","1.80"]
["","Type","","","","R-410A"]
["Toimintalämpötila-alue","Asennustila","","Min.","°C","5.00"]
["","","","Maks.","°C","30.0"]
["","Lämmitys","Vesi","Maks.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Suolavesipuoli","","Min.","°C","-5.00"]
["","","","Maks.","°C","20.0"]
["","Kuuma käyttövesi","Vesi","Maks.","°C","55 (7), 60 (9)"]
["","","","Min.","°C","25 (7), 25 (9)"]
["Ottoteho","Nom.","","","kW","2.38 (1), 2.89 (2)"]
["Äänen tehotaso","Nimell.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Mitat","Yksikkö","","Leveys","mm","600"]
["","","","Syvyys","mm","728"]
["","","","Korkeus","mm","1,730"]
["Casing","Material","","","","Pinnoitettu metallilevy"]
["","Väri","","","","Valkoinen"]
["Säiliö","Vesitilavuus","","","l","180"]
["","Korroosionsuojaus","","","","Anodi"]
["","Eristys","","Lämpöhäviö","kWh / 24h","1.36 (4)"]
["Paino","Yksikkö","","","kg","210"]
["Tilojen lämmitys","Keskimäär. ilmaston veden lähtö 35°C","Yleistä","ηs (kausittainen tilojen lämmityksen tehokkuus)","%","194"]
["","","","Kausittainen tilojen lämmityksen tehokk.luokka","","A+++"]
["","","","SCOP","","5.06"]
["","Keskimäär. ilmaston veden lähtö 55 °C","Yleistä","Kausittainen tilojen lämmityksen tehokk.luokka","","A++"]
["","","","ηs (kausittainen tilojen lämmityksen tehokkuus)","%","139"]
["","","","SCOP","","3.68"]
["Lämmitysteho","Nimell.","","","kW","10.3 (1), 9.20 (2)"]
["","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Maks.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","Phase","","","","3~"]
["","Name","","","","9W"]
["","Taajuus","","","Hz","50"]
["","Jännite","","","V","400"]
["Virta","Suositeltu sulakekoko","","","A","25"]
["Huomautukset","","","","","(1) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)"]
["","","","","","(2) - EWB/LWB 0°C/-3°C - LWC 45°C (DT=5°C)"]
["","","","","","(3) - 40 % propyleeniglykolia"]
["","","","","","(4) - Lämpöhäviöt EN12897 mukaan"]
["","","","","","(5) - Sisältäen putkisto + PHE + varalämmitin / ilman paisuntasäiliötä"]
["","","","","","(6) - Äänenpaineen taso mitataan mikrofonilla 1 m etäisyydeltä yksiköstä. Arvo on suhteellinen ja määräytyy etäisyyden ja ympäristön akustiikan mukaan."]
["","","","","","(7) - Lämpöpumpulla"]
["","","","","","(8) - Lämpöpumpulla + varalämmittimellä"]
["","","","","","(9) - Varalämmittimellä"]