{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSH-E"]
[]
[]
[]
[]
["","","","","","EHSH04P30EG","EHSH04P30EF","EHSH08P30EG","EHSH08P50EG","EHSH08P30EF","EHSH08P50EF"]
["Kotelo","Väri","","","","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)"]
["","Materiaali","","","","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni"]
["Mitat","Yksikkö","","Korkeus","mm","1,891","1,892","1,891","1,910","1,892","1,905"]
["","","","Leveys","mm","594","594","594","792","594","792"]
["","","","Syvyys","mm","644","644","644","817","644","812"]
["Paino","Yksikkö","","","kg","77.0","77","77.0","97.0","77","107"]
["PED","Luokka","","","","Art4.3","Art4.3","Art4.3","Art4.3","Art4.3","Art4.3"]
["Kylmäaine","Tyyppi","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675.0","675","675.0","675.0","675","675"]
["","Täytösmäärä","","","kg","1.50","1.5","1.50","1.50","1.5","1.5"]
["Äänen tehotaso","Nimell.","","","dBA","39","39","39","39","39","39"]
["Toimintalämpötila-alue","Lämmitys","Vesi","Min.","°C","18","18","18","18","18","18"]
["","","","Maks.","°C","65","65","65","65","65","65"]
["","Jäähdytys","Ympäristö","Min.","°CDB","10","10","10","10","10","10"]
["","","Vesi","Min.","°C","5","5","5","5","5","5"]
["","","","Maks.","°C","22","22","22","22","22","22"]
["Virransyöttö","Vaihe","","","","1~","1~","1~","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50","50","50","50"]
["","Jännite","","","V","230","230","230","230","230","230"]
["Huomautukset","","","","","(1) - Lämpöhäviöt EN12897 mukaan","(1) - Lämpöhäviöt EN12897 mukaan","(1) - Lämpöhäviöt EN12897 mukaan","(1) - Lämpöhäviöt EN12897 mukaan","(1) - Lämpöhäviöt EN12897 mukaan","(1) - Lämpöhäviöt EN12897 mukaan"]