{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-D3"]
[]
[]
[]
[]
["","","","","","EHSX04P30DA3","EHSX04P50DA3","EHSX08P30DA3"]
["Kotelo","Väri","","","","Liike valkoinen (RAL9016) / tummanharmaa (RAL7011)","Liike valkoinen (RAL9016) / tummanharmaa (RAL7011)","Liike valkoinen (RAL9016) / tummanharmaa (RAL7011)"]
["","Materiaali","","","","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni"]
["Mitat","Yksikkö","","Korkeus","mm","1891","1896","1891"]
["","","","Leveys","mm","595","790","595"]
["","","","Syvyys","mm","615","790","615"]
["Paino","Yksikkö","","","kg","73.0","93.0","73.0"]
["PED","Luokka","","","","art. 3.3","art. 3.3","art. 3.3"]
["Kylmäaine","Tyyppi","","","","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0"]
["","Täytösmäärä","","","kg","1.50","1.50","1.50"]
["Äänen tehotaso","Nimell.","","","dBA","39","39","39"]
["Toimintalämpötila-alue","Lämmitys","Vesi","Min.","°C","18","18","18"]
["","","","Maks.","°C","65","65","65"]
["","Jäähdytys","Ympäristö","Min.","°CDB","10","10","10"]
["","","Vesi","Min.","°C","5","5","5"]
["","","","Maks.","°C","22","22","22"]
["Virransyöttö","Vaihe","","","","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50"]
["","Jännite","","","V","230","230","230"]
["Sähkölämmitin","Syöttöjännite","","Nimi","","3V / 9W","3V / 9W","3V / 9W"]
["","","","Vaihe","","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Taajuus","Hz","50","50","50"]
["Huomautukset","","","","","(1) - Lämpöhäviöt EN12897 mukaan","(1) - Lämpöhäviöt EN12897 mukaan","(1) - Lämpöhäviöt EN12897 mukaan"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","","(5) - Kuumenna säiliö vain lämpöpumpun avulla, ei sähkölämmittimellä"]