{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E6VG / ERGA-EV"]
[]
[]
[]
[]
["","","","","","EHVX04S18EA6VG / ERGA04EAV3","EHVX04S23EA6VG / ERGA04EAV3"]
["Lämmitysteho","Nimell.","","","kW","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)"]
["Jäähdytysteho","Nimell.","","","kW","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)"]
["Ottoteho","Lämmitys","","Nimell.","kW","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)"]
["","Jäähdytys","","Nimell.","kW","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)"]
["","Kuuma käyttövesi 10°C...50 °C","","Nim.","kWh","2.48","3.01"]
["Lämpenemisaika 10°C...50 °C","hr","","","","1 h 28 min","1 h 40 min"]
["COP","","","","","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)"]
["EER","","","","","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)"]
["Lämminvesivaraaja","Yleistä","","Ilmoitettu kuormitusprofiili","","L","XL"]
["","Keskimääräinen ilmasto","","Vedenlämmityksen energiatehokkuusluokka","","A+","A+"]
["Tilojen lämmitys","Keskimäär. ilmaston veden lähtö 55 °C","Yleistä","SCOP","","3.29","3.29"]
["","","","Kausittainen tilojen lämmityksen tehokk.luokka","","A++","A++"]
["","Keskimäär. ilmaston veden lähtö 35°C","Yleistä","SCOP","","4.54","4.54"]
["","","","Kausittainen tilojen lämmityksen tehokk.luokka","","A+++","A+++"]
["Huomautukset","","","","","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Ehto 1: jäähdytys Ta 35°C - LWE 18°C (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Ehto 2: jäähdytys Ta 35°C - LWE 7°C ( DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]