{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELSH-E"]
[]
[]
[]
[]
["","","","","","ELSH12P30EF","ELSH12P50EF","ELSH12P30EG","ELSH12P50EG"]
["Kotelo","Väri","","","","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)","Liikennevalkoinen (RAL9016) / Liikennemusta (RAL9017)"]
["","Materiaali","","","","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni","Iskunkestävä polypropeeni"]
["Mitat","Yksikkö","","Korkeus","mm","1,893","1,910","1,891","1,910"]
["","","","Leveys","mm","594","792","594","792"]
["","","","Syvyys","mm","680","817","680","817"]
["Paino","Yksikkö","","","kg","76.0","91.0","91.0","112"]
["PED","Luokka","","","","Luokka II","Luokka II","Luokka II","Luokka II"]
["Kylmäaine","Tyyppi","","","","R-32","R-32","R-32","R-32"]
["Äänen tehotaso","Nimell.","","","dBA","44.7","44.7","44.7","44.7"]
["Äänenpaineen taso","Nimell.","","","dBA","36.8","36.8","36.8","36.8"]
["Toimintalämpötila-alue","Lämmitys","Vesi","Min.","°C","15 (3)","15 (3)","15 (3)","15 (3)"]
["","","","Maks.","°C","65 (3)","65 (3)","65 (3)","65 (3)"]
["","Jäähdytys","Ympäristö","Min.","°CDB","10 (3)","10 (3)","10 (3)","10 (3)"]
["","","Vesi","Min.","°C","5 (3)","5 (3)","5 (3)","5 (3)"]
["","","","Maks.","°C","22 (3)","22 (3)","22 (3)","22 (3)"]
["Virransyöttö","Vaihe","","","","1~","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50","50"]
["","Jännite","","","V","230","230","230","230"]
["Huomautukset","","","","","(1) - Toiminta-alue ulottuu pieniin virtaamiin toimintatilasta riippuen – katso ESP-käyrä.","(1) - Toiminta-alue ulottuu pieniin virtaamiin toimintatilasta riippuen – katso ESP-käyrä.","(1) - Toiminta-alue ulottuu pieniin virtaamiin toimintatilasta riippuen – katso ESP-käyrä.","(1) - Toiminta-alue ulottuu pieniin virtaamiin toimintatilasta riippuen – katso ESP-käyrä."]
["","","","","","(2) - Lämpöhäviöt EN12897 mukaan","(2) - Lämpöhäviöt EN12897 mukaan","(2) - Lämpöhäviöt EN12897 mukaan","(2) - Lämpöhäviöt EN12897 mukaan"]
["","","","","","(3) - Lisätietoja on toimintalämpötila-alueen piirroksessa","(3) - Lisätietoja on toimintalämpötila-alueen piirroksessa","(3) - Lisätietoja on toimintalämpötila-alueen piirroksessa","(3) - Lisätietoja on toimintalämpötila-alueen piirroksessa"]