{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EVH7"]
[]
[]
[]
[]
["","","","","","ERGA08EAV3H7"]
["Mitat","Yksikkö","","Korkeus","mm","740"]
["","","","Leveys","mm","884"]
["","","","Syvyys","mm","388"]
["Paino","Yksikkö","","","kg","58.5"]
["Toimintalämpötila-alue","Jäähdytys","","Min.","°CDB","10"]
["","","","Maks.","°CDB","43"]
["","Kuuma käyttövesi","","Min.","°CDB","-25"]
["","","","Maks.","°CDB","35"]
["Äänen tehotaso","Lämmitys","","Nimell.","dBA","62 (1)"]
["","Jäähdytys","","Nimell.","dBA","62 (1)"]
["Äänenpaineen taso","Lämmitys","","Nimell.","dBA","49 (1)"]
["","Jäähdytys","","Nimell.","dBA","50 (1)"]
["Kylmäaine","Tyyppi","","","","R-32"]
["","GWP","","","","675.0"]
["","Täytösmäärä","","","tCO2Eq","1.01"]
["","Täytösmäärä","","","kg","1.50"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6"]
["","Kaasu","","Ulkohalkaisija","mm","15.9"]
["Putkistoliitännät","Tyhjennys","","Ulkohalkaisija","mm","18"]
["","Korkeusero","IU - OU","Maks.","m","30.0"]
["Putkiliitännät","Lämmöneristys","","","","Sekä neste- että kaasuputket"]
["Virransyöttö","Nimi","","","","V3"]
["","Vaihe","","","","1N~"]
["Syöttöjännite","Taajuus","","","Hz","50"]
["","Jännite","","","V","230"]
["Virta","Suositeltu sulakekoko","","","A","25"]
["Huomautukset","","","","","(1) - Jäähdytys Ta 35°C - LWE 18℃ (DT = 5°C); lämmitys Ta DB/WB 7°C/6°C - LWC 35℃ (DT = 5°C)"]